

[Version]
signature="$CHICAGO$" ;all windows os
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%PSH%
DriverVer=08/10/2007,1.0.3.7
CatalogFile=716xBDA.cat
CatalogFile.NTAMD64 = AMD64\716xBDA.cat
CatalogFile.NTIA64  = IA64\716xBDA.cat

[Manufacturer]
%PSH%=DTV-DVB, NTAMD64, NTIA64

[DTV-DVB]
%6090.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00271822 ;6090
%6091.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00321822 ;6091
%6050.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00331822 ;6050
%6051.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00411822 ;6051
%Nunzio_6090.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00371822 ;Nunzio_6090
%3071.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7160&SUBSYS_00391822 ;3071
%1028.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7160&SUBSYS_00441822 ;1028

[DTV-DVB.NTAMD64]
%6090.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00271822 ;6090
%6091.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00321822 ;6091
%6050.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00331822 ;6050
%6051.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00411822 ;6051
%Nunzio_6090.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00371822 ;Nunzio_6090
%3071.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7160&SUBSYS_00391822 ;3071
%1028.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7160&SUBSYS_00441822 ;1028

[DTV-DVB.NTIA64]
%6090.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00271822 ;6090
%6091.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00321822 ;6091
%6050.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00331822 ;6050
%6051.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00411822 ;6051
%Nunzio_6090.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7162&SUBSYS_00371822 ;Nunzio_6090
%3071.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7160&SUBSYS_00391822 ;3071
%1028.DeviceDesc%=716xBDA,PCI\VEN_1131&DEV_7160&SUBSYS_00441822 ;1028

[DestinationDirs]
716xBDA.CopyFiles=10,system32\drivers ; be aware not to use 12 as the drivers directory, 
                                       ; as driver will not work anymore in W98

[SourceDisksNames]
1 = %AVSTRM_INSTALLATION_DISK%,,

[SourceDisksNames.AMD64]
1 = %AVSTRM_INSTALLATION_DISK%, 716xBDA.inf, , \AMD64

[SourceDisksNames.IA64]
1 = %AVSTRM_INSTALLATION_DISK%, 716xBDA.inf, , \IA64

[SourceDisksFiles]
716xCoInstaller.dll=1
716xBDA.sys=1

[716xBDA.CopyCoInst]
716xCoInstaller.dll

[716xBDA.CopyFiles]
716xBDA.sys

;
;*** initialization and registry entries
;

[716xBDA.CoInstallers]
CopyFiles = 716xBDA.CopyCoInst
AddReg = 716xBDA.CoInstaller_AddReg

[716xBDA.ntx86.CoInstallers]
CopyFiles = 716xBDA.CopyCoInst
AddReg = 716xBDA.CoInstaller_AddReg

[716xBDA.CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000,"716xCoInstaller.dll, CoInstallerEntry"

[716xBDA]
AlsoInstall=KS.Registration(ks.inf), WDMAUDIO.Registration(wdmaudio.inf), KSCAPTUR.Registration(kscaptur.inf), BDA.Installation(bda.inf)
CopyFiles=716xBDA.CopyFiles
AddReg=716xBDA.AddReg

[716xBDA.ntx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles=716xBDA.CopyFiles
AddReg=716xBDA.AddReg

[716xBDA.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles=716xBDA.CopyFiles
AddReg=716xBDA.AddReg

[716xBDA.NTIA64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles=716xBDA.CopyFiles
AddReg=716xBDA.AddReg

[716xBDA.Services]
AddService=716xBDA, 0x00000002, 716xBDA.ServiceInstall

[716xBDA.ntx86.Services]
AddService=716xBDA, 0x00000002, 716xBDA.ServiceInstall

[716xBDA.NTAMD64.Services]
AddService=716xBDA, 0x00000002, 716xBDA.ServiceInstall, 716xBDA.EventInstall

[716xBDA.NTIA64.Services]
AddService=716xBDA, 0x00000002, 716xBDA.ServiceInstall, 716xBDA.EventInstall

[716xBDA.ServiceInstall]
DisplayName=%DISPLAY_NAME%
Description=%SERVICE_DESCRIPTION%
ServiceType=%SERVICE_KERNEL_DRIVER%
StartType=%SERVICE_DEMAND_START%
ErrorControl=%SERVICE_ERROR_IGNORE%
ServiceBinary=%12%\716xBDA.sys
; [StartName=driver-object-name]
; [AddReg=add-registry-section[, add-registry-section] ...]
; [DelReg=del-registry-section[, del-registry-section] ...]
; [BitReg=bit-registry-section[,bit-registry-section] ...]
; [LoadOrderGroup=load-order-group-name]
; [Dependencies=depend-on-item-name[,depend-on-item-name]...]

[716xBDA.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,716xBDA.sys

;Disabe HID driver install
HKR,"ENUM\Device1",pnpid,,"716xHID.VIRTUAL"

; audio capture registry entries

HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,716xBDA.SYS

HKR,Drivers,SubClasses,,"wave,mixer"

HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv

HKR,Drivers\wave\wdmaud.drv,Description,,"Europa audio capture device"
HKR,Drivers\mixer\wdmaud.drv,Description,,"Europa audio capture device"

; Setting FM radio of the Silicon tuner via SIF (GPIO 21 in use/ 5.5MHz)
HKR, "Audio", "FM Radio IF",0x00010001,0x729555


;++++++++++++++++++++++++++ For 716x Device ++++++++++++++++++++++++++++++++++++
; Device_Name (MAX 32 bytes)
;HKR,"DriverData","Device_Name",0x00010000, "716x PCIe Capture"

; SupportHWInfo (MAX 32 bytes)
;HKR,"DriverData","SupportHWInfo",0x00010000, "PCIe_6IN1_2DVBS_2DVBT_HYBRID"

; IR Stanard (RC-5:0x00, NEC:0x01)
HKR,"DriverData","IR_Standard",0x00010001, 0x00,0x00,0x00,0x00
;HKR,"DriverData","IR_Standard",0x00010001, 0x01,0x00,0x00,0x00

; IR system code checklist1 (RC-5: 0x001B, NEC: 0x00ff)
HKR,"DriverData","IRSYSCODECHECK1",0x00010001, 0x1B,0x00,0x00,0x00
;HKR,"DriverData","IRSYSCODECHECK1",0x00010001, 0xff,0x00,0x00,0x00

; //Mapping RC table for DTV-DVB
HKR,"DriverData","RC_Configuration",0x00010001, 0x00,0x00,0x00,0x00
; //Mapping RC table for Cyberlink
;HKR,"DriverData","RC_Configuration",0x00010001, 0x01,0x00,0x00,0x00
; //Mapping RC table for IVI
;HKR,"DriverData","RC_Configuration",0x00010001, 0x02,0x00,0x00,0x00
; //Mapping RC table for MCE
;HKR,"DriverData","RC_Configuration",0x00010001, 0x03,0x00,0x00,0x00
; //Mapping RC table for NEW TH HID RC
;HKR,"DriverData","RC_Configuration",0x00010001, 0x04,0x00,0x00,0x00
; //Mapping RC table for Custom
;HKR,"DriverData","RC_Configuration",0x00010001, 0x05,0x00,0x00,0x00
; //Mapping RC table for DNTVLive HID RC
;HKR,"DriverData","RC_Configuration",0x00010001, 0x10,0x00,0x00,0x00
; //Disable RC
;HKR,"DriverData","RC_Configuration",0x00010001, 0xFF,0xFF,0x00,0x00
;-------------------------- For 716x Device ------------------------------------

;++++++++++++++++++++++++++ For DVB-T Device <1> ++++++++++++++++++++++++++++++++++++
;RF input selection, 0:Master  1:Slave
HKR,"DriverData0","DigitalTV-RF-In",0x00010001, 0x00,0x00,0x00,0x00

; //As it is, no change
HKR,"DriverData0","MCE_FreqTranslate",0x00010001, 0x00,0x00,0x00,0x00
; //Fixed 6 MHz Freq table
;HKR,"DriverData0","MCE_FreqTranslate",0x00010001, 0x06,0x00,0x00,0x00
; //Fixed 7 MHz Freq table
;HKR,"DriverData0","MCE_FreqTranslate",0x00010001, 0x07,0x00,0x00,0x00
; //Fixed 8 MHz Freq table
;HKR,"DriverData0","MCE_FreqTranslate",0x00010001, 0x08,0x00,0x00,0x00

; //As it is, no change
HKR,"DriverData0","FixedBandwidth",0x00010001, 0x00,0x00,0x00,0x00
; //VHF in 7 MHz, UHF in 8 MHz
;HKR,"DriverData0","FixedBandwidth",0x00010001, 0x01,0x00,0x00,0x00
; //Fixed 6 MHz
;HKR,"DriverData0","FixedBandwidth",0x00010001, 0x06,0x00,0x00,0x00
; //Fixed 7 MHz
;HKR,"DriverData0","FixedBandwidth",0x00010001, 0x07,0x00,0x00,0x00
; //Fixed 8 MHz
;HKR,"DriverData0","FixedBandwidth",0x00010001, 0x08,0x00,0x00,0x00

; //167KHz will be scanned
HKR,"DriverData0","ShiftFreqScan",0x00010001, 0x00,0x00,0x00,0x00
; //Don't scan +-167KHz, just return lock failure
;HKR,"DriverData0","ShiftFreqScan",0x00010001, 0x01,0x00,0x00,0x00
;-------------------------- For DVB-T Device <1> ------------------------------------

;++++++++++++++++++++++++++ For DVB-T Device <2> ++++++++++++++++++++++++++++++++++++
;RF input selection, 0:Master  1:Slave
HKR,"DriverData1","DigitalTV-RF-In",0x00010001, 0x00,0x00,0x00,0x00

; //As it is, no change
HKR,"DriverData1","MCE_FreqTranslate",0x00010001, 0x00,0x00,0x00,0x00
; //Fixed 6 MHz Freq table
;HKR,"DriverData1","MCE_FreqTranslate",0x00010001, 0x06,0x00,0x00,0x00
; //Fixed 7 MHz Freq table
;HKR,"DriverData1","MCE_FreqTranslate",0x00010001, 0x07,0x00,0x00,0x00
; //Fixed 8 MHz Freq table
;HKR,"DriverData1","MCE_FreqTranslate",0x00010001, 0x08,0x00,0x00,0x00

; //As it is, no change
HKR,"DriverData1","FixedBandwidth",0x00010001, 0x00,0x00,0x00,0x00
; //VHF in 7 MHz, UHF in 8 MHz
;HKR,"DriverData1","FixedBandwidth",0x00010001, 0x01,0x00,0x00,0x00
; //Fixed 6 MHz
;HKR,"DriverData1","FixedBandwidth",0x00010001, 0x06,0x00,0x00,0x00
; //Fixed 7 MHz
;HKR,"DriverData1","FixedBandwidth",0x00010001, 0x07,0x00,0x00,0x00
; //Fixed 8 MHz
;HKR,"DriverData1","FixedBandwidth",0x00010001, 0x08,0x00,0x00,0x00

; //167KHz will be scanned
HKR,"DriverData1","ShiftFreqScan",0x00010001, 0x00,0x00,0x00,0x00
; //Don't scan +-167KHz, just return lock failure
;HKR,"DriverData1","ShiftFreqScan",0x00010001, 0x01,0x00,0x00,0x00
;-------------------------- For DVB-T Device <2> ------------------------------------

;++++++++++++++++++++++++++ For DVB-S Device <1> ++++++++++++++++++++++++++++++++++++
;RF input selection, 0:Master  1:Slave
HKR,"DriverData2","DigitalTV-RF-In",0x00010001, 0x00,0x00,0x00,0x00

; Local Oscillator Frequency (LOF)
; 0: If BDAIoctl set,use BDAIoctl only, else use standard BDA interface
HKR,"DriverData2","LNBLOF",0x00010001, 0x00,0x00,0x00,0x00
; 3: Use INF setting only!
;HKR,"DriverData2","LNBLOF",0x00010001, 0x03,0x00,0x00,0x00

; LNBLOFLowBand = 5150  MHz
HKR,"DriverData2","LNBLOFLowBand",0x00010001, 0x1E,0x14,0x00,0x00
; LNBLOFHighBand = 5750 MHz
HKR,"DriverData2","LNBLOFHighBand",0x00010001, 0x76,0x16,0x00,0x00
; LNBLOF Low/High band switch, 0 MHz
HKR,"DriverData2","LNBLOFHiLoSwitch",0x00010001, 0x0,0x0,0x00,0x00

; DiSEqC Selection
; 0: Normal
HKR,"DriverData2","DiSEqC",0x00010001, 0x00,0x00,0x00,0x00
; 1: DiSEqC A
;HKR,"DriverData2","DiSEqC",0x00010001, 0x01,0x00,0x00,0x00
; 2: DiSEqC B
;HKR,"DriverData2","DiSEqC",0x00010001, 0x02,0x00,0x00,0x00
; 3: DiSEqC C
;HKR,"DriverData2","DiSEqC",0x00010001, 0x03,0x00,0x00,0x00
; 4: DiSEqC D
;HKR,"DriverData2","DiSEqC",0x00010001, 0x04,0x00,0x00,0x00

; LNB Power
; 0: OFF
;HKR,"DriverData2","LNBPower",0x00010001, 0x00,0x00,0x00,0x00
; 1: ON
HKR,"DriverData2","LNBPower",0x00010001, 0x01,0x00,0x00,0x00

; 22k Tone
; 0: ON/OFF by LNB switch frequency
;HKR,"DriverData2","Tone",0x00010001, 0x00,0x00,0x00,0x00
; 1: OFF
HKR,"DriverData2","Tone",0x00010001, 0x01,0x00,0x00,0x00
; 2: ON
;HKR,"DriverData2","Tone",0x00010001, 0x02,0x00,0x00,0x00

; Tone and Data Burst
; 0: Tone and data burst off
HKR,"DriverData2","ToneDataBurst",0x00010001, 0x00,0x00,0x00,0x00
; 1: Tone burst on
;HKR,"DriverData2","ToneDataBurst",0x00010001, 0x01,0x00,0x00,0x00
; 2: Data burst on
;HKR,"DriverData2","ToneDataBurst",0x00010001, 0x02,0x00,0x00,0x00

; TSGenSimulator
; 0:Disabled, 1:DVB-S, 2:DVB-T, 4:DVB-C, 8:ATSC 16:MCE DVB-T
;HKR,"DriverData2","TSGenSimulator",0x00010001, 0x11,0x00,0x00,0x00
;-------------------------- For DVB-S Device <1> ------------------------------------

;++++++++++++++++++++++++++ For DVB-S Device <2> ++++++++++++++++++++++++++++++++++++
;RF input selection, 0:Master  1:Slave
HKR,"DriverData3","DigitalTV-RF-In",0x00010001, 0x00,0x00,0x00,0x00

; Local Oscillator Frequency (LOF)
; 0: If BDAIoctl set,use BDAIoctl only, else use standard BDA interface
HKR,"DriverData3","LNBLOF",0x00010001, 0x00,0x00,0x00,0x00
; 3: Use INF setting only!
;HKR,"DriverData3","LNBLOF",0x00010001, 0x03,0x00,0x00,0x00

; LNBLOFLowBand = 9750  MHz
HKR,"DriverData3","LNBLOFLowBand",0x00010001, 0x16,0x26,0x00,0x00
; LNBLOFHighBand = 10600 MHz
HKR,"DriverData3","LNBLOFHighBand",0x00010001, 0x68,0x29,0x00,0x00
; LNBLOF Low/High band switch, 11700 MHz
HKR,"DriverData3","LNBLOFHiLoSwitch",0x00010001, 0xb4,0x2d,0x00,0x00

; DiSEqC Selection
; 0: Normal
HKR,"DriverData3","DiSEqC",0x00010001, 0x00,0x00,0x00,0x00
; 1: DiSEqC A
;HKR,"DriverData3","DiSEqC",0x00010001, 0x01,0x00,0x00,0x00
; 2: DiSEqC B
;HKR,"DriverData3","DiSEqC",0x00010001, 0x02,0x00,0x00,0x00
; 3: DiSEqC C
;HKR,"DriverData3","DiSEqC",0x00010001, 0x03,0x00,0x00,0x00
; 4: DiSEqC D
;HKR,"DriverData3","DiSEqC",0x00010001, 0x04,0x00,0x00,0x00

; LNB Power
; 0: OFF
;HKR,"DriverData3","LNBPower",0x00010001, 0x00,0x00,0x00,0x00
; 1: ON
HKR,"DriverData3","LNBPower",0x00010001, 0x01,0x00,0x00,0x00

; 22k Tone
; 0: ON/OFF by LNB switch frequency
;HKR,"DriverData3","Tone",0x00010001, 0x00,0x00,0x00,0x00
; 1: OFF
HKR,"DriverData3","Tone",0x00010001, 0x01,0x00,0x00,0x00
; 2: ON
;HKR,"DriverData3","Tone",0x00010001, 0x02,0x00,0x00,0x00

; Tone and Data Burst
; 0: Tone and data burst off
HKR,"DriverData3","ToneDataBurst",0x00010001, 0x00,0x00,0x00,0x00
; 1: Tone burst on
;HKR,"DriverData3","ToneDataBurst",0x00010001, 0x01,0x00,0x00,0x00
; 2: Data burst on
;HKR,"DriverData3","ToneDataBurst",0x00010001, 0x02,0x00,0x00,0x00

; TSGenSimulator
; 0:Disabled, 1:DVB-S, 2:DVB-T, 4:DVB-C, 8:ATSC 16:MCE DVB-T
;HKR,"DriverData3","TSGenSimulator",0x00010001, 0x11,0x00,0x00,0x00
;-------------------------- For DVB-S Device <2> ------------------------------------


; add audio input and output pinnames

HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"

[716xBDA.EventInstall]
AddReg = 716xBDAEvent_AddReg

[716xBDAEvent_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\716xBDA.sys"
HKR,,TypesSupported,0x00010001,7

;
;*** strings, GUIDs and names
;

[Strings]

; Proxy GUIDs

KSProxy.CLSID   = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSXBar.CLSID    = "{71F96460-78F3-11d0-A18C-00A0C9118956}"
KSTVAudio.CLSID = "{71F96462-78F3-11d0-A18C-00A0C9118956}"
KSTvTune.CLSID  = "{266EEE40-6C63-11cf-8A03-00AA006ECB65}"

; Category GUIDs

KSCATEGORY_MULTIPLEXER            = "{7A5DE1D3-01A1-452c-B481-4FA2B96271E8}"
KSCATEGORY_ENCODER                = "{19689BF6-C384-48fd-AD51-90E58C79F70B}"
KSCATEGORY_CAPTURE                = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO                  = "{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_AUDIO                  = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"

; Our Pin Name GUIDs

VAMP_ANLG_AUDIO_IN_PIN   = "{7BB284B9-714D-493d-A101-B1B028E782BD}"
VAMP_ANLG_AUDIO_OUT_PIN  = "{5582E657-E596-42b5-9DB3-541B27A2355F}"
VAMP_ANLG_AUDIO_I2S_PIN  = "{C2E46358-F032-4d88-B802-06B59D162730}"
VAMP_ANLG_VIDEO_ITU_PIN  = "{82631A2E-403C-4581-A4B0-EC173D004410}"

; Our Filter GUIDs

VAMP_MPG_ENCODER_FILTER  = "{949607F9-0DA5-4099-982E-D91DE6150B00}"
VAMP_ANLG_AUDIO_FILTER   = "{F3B951E7-8619-4ff3-91CA-03910E4BB900}"
VAMP_ANLG_CAP_FILTER     = "{BBEFB6C7-2FC4-4139-BB8B-A58BBA724000}"

; system defines

SERVICE_BOOT_START     = 0x0 
SERVICE_SYSTEM_START   = 0x1 
SERVICE_AUTO_START     = 0x2 
SERVICE_DEMAND_START   = 0x3 
SERVICE_DISABLED       = 0x4 

SERVICE_KERNEL_DRIVER  = 0x1 
SERVICE_ERROR_IGNORE   = 0x0 
SERVICE_ERROR_NORMAL   = 0x1 
SERVICE_ERROR_SEVERE   = 0x2
SERVICE_ERROR_CRITICAL = 0x3 

FLG_REGSVR_DLLREGISTER = 0x00000001

;Our strings

PSH="DTV-DVB"
6090.DeviceDesc             = "DTV-DVB 6090 PCIe Capture Device with HID "
Nunzio_6090.DeviceDesc      = "DTV-DVB Nunzio_6090 PCIe Capture Device with HID"
6091.DeviceDesc             = "DTV-DVB 6091 PCIe Capture Device with HID"
6050.DeviceDesc             = "DTV-DVB 6050 PCIe Capture Device with HID"
6051.DeviceDesc             = "DTV-DVB 6051 PCIe Capture Device with HID"
3071.DeviceDesc             = "DTV-DVB 3071 PCIe Capture Device with HID"
1028.DeviceDesc             = "DTV-DVB 1028 PCIe Capture Device with HID"
AVSTRM_INSTALLATION_DISK    = "716xBDA installation disk"
DISPLAY_NAME                = "716xBDA service"
SERVICE_DESCRIPTION         = "The PCIe capture driver"
