;
;   Installation inf file for 6090 adapter HID driver
;

[Version]
Signature="$CHICAGO$"
Class=HIDClass
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
Provider=%DTV-DVB%
DriverVer=08/10/2007,1.0.1.5
CatalogFile 	= 716xHID.cat
CatalogFile.NTAMD64 = AMD64\716xHID.cat
CatalogFile.NTIA64  = IA64\716xHID.cat

[Manufacturer]
%MfgName% = DTV-DVB, NTAMD64, NTIA64

[DTV-DVB]
%716xHID.DeviceDesc%=716xHID.Device,AVSTREAM\716xHID.VIRTUAL
%716xHID1.DeviceDesc%=716xHID.Device1,AVSTREAM\716xHID.VIRTUAL

[DTV-DVB.NTAMD64]
%716xHID.DeviceDesc%=716xHID.Device,AVSTREAM\716xHID.VIRTUAL
%716xHID1.DeviceDesc%=716xHID.Device1,AVSTREAM\716xHID.VIRTUAL

[DTV-DVB.NTIA64]
%716xHID.DeviceDesc%=716xHID.Device,AVSTREAM\716xHID.VIRTUAL
%716xHID1.DeviceDesc%=716xHID.Device1,AVSTREAM\716xHID.VIRTUAL

[DestinationDirs]
716xHID.CopyDrivers = 10,System32\Drivers 

[SourceDisksNames]
1 = %INSTALLATION_DISK%,,

[SourceDisksNames.AMD64]
1 = %INSTALLATION_DISK%, 716xHID.inf, , \AMD64

[SourceDisksNames.IA64]
1 = %INSTALLATION_DISK%, 716xHID.inf, , \IA64

[SourceDisksFiles]
716xHID.sys = 1

[ControlFlags]
ExcludeFromSelect	= *
ExcludeFromSelect.NT	= *

[716xHID.Device]
CopyFiles = 716xHID.CopyDrivers
AddReg    = 716xHID.AddReg

[716xHID.Device.NT]
CopyFiles = 716xHID.CopyDrivers
AddReg    = 716xHID.AddReg

[716xHID.Device.NT.Services]
AddService = 716xHID,0x00000002,716xHID.AddService



[716xHID.Device1]
CopyFiles = 716xHID.CopyDrivers
AddReg    = 716xHID.AddReg1

[716xHID.Device1.NT]
CopyFiles = 716xHID.CopyDrivers
AddReg    = 716xHID.AddReg1

[716xHID.Device1.NT.Services]
AddService = 716xHID,0x00000002,716xHID.AddService


[716xHID.AddService]
DisplayName     = %716xHID.FriendlyName%
ServiceType     = 1                  ; SERVICE_KERNEL_DRIVER
StartType       = 3                  ; SERVICE_DEMAND_START
ErrorControl    = 0                  ; SERVICE_ERROR_IGNORE
ServiceBinary   = %10%\system32\drivers\716xHID.sys
LoadOrderGroup  = Extended Base

[716xHID.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,716xHID.sys

;0:Twinhan Hotkey table only, 1:All RC table
HKR,"DriverData","RC_Report",0x00010001, 0x00,0x00, 0x00, 0x00

[716xHID.AddReg1]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,716xHID.sys

;0:Twinhan Hotkey table only, 1:All RC table
HKR,"DriverData","RC_Report",0x00010001, 0x01,0x00, 0x00, 0x00

;Configurable RC Hot keys 
; Scan code mappings.
; Format: SCANCODE_nn = 0xii, 0xjj, 0xkk, 0xll
;   nn: hex value of scan code (Please reference DTV-DVB RC table)
;   ii: first virtual key value
;   jj: ctrl virtual key value
;   kk: shift virtual key value
;   ll: alt virtual key value
; Note: 1) Refer to MSDN for virtual key values (keyword: "VK_")
;       2) Maximum three key combination supported now
;
;HKR,"DriverData","RC_Scancode_00",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_01",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_02",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_03",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_04",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_05",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_06",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_07",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_08",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_09",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_0A",0x00010001, 0x00,0x00, 0x00, 0x00
;.....
;.....
;HKR,"DriverData","RC_Scancode_71",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_72",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_73",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_74",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_75",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_76",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_77",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_78",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7A",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7B",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7C",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7D",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7E",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7F",0x00010001, 0x00,0x00, 0x00, 0x00


[716xHID.CopyDrivers]
716xHID.sys

[Strings]
DTV-DVB				= "DTV-DVB"
MfgName				= "DTV-DVB"

716xHID.DeviceDesc		= "716xHID - PCIe HID Device (For TH RC only)"
716xHID1.DeviceDesc	    = "716xHID - PCIe HID Device (Support all RC's)"
716xHID.FriendlyName	= "716xHID - PCIe HID Driver"
INSTALLATION_DISK		= "716xHID - PCIe HID Installation Disk"