;******************************************************************
; Copyright (C) 1996-1998, Rockwell Semiconductor Systems, Inc.   
; Copyright (C) 1999-2010, Conexant Systems Inc.                   
;******************************************************************
;    cphdapo.inf >> TPUNPEBy.inf
;
;Abstract:
;    INF file for installing the Conexant Function Driver for 
;    Pebble High Definition Audio Device
;                               
;******************************************************************

[Version]
Signature="$Windows NT$"
Class=MEDIA
ClassGuid={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=Conexant
CatalogFile = TPUNPEBy.cat
DriverVer = 10/20/2010, 4.95.48.50
 
[DestinationDirs]
DefaultDestDir      =10; dirid = \system32\drivers
HdAudModel.Copyfiles =10,system32\drivers
CoInstaller_CopyFiles=10,system32
Uninstall.CopyFiles=16422,CONEXANT\%UIPATH%
SfxFx.CopyList=11     ; %windir%\system32

[SourceDisksNames]
222=%DiskId1%,,,

[SourceDisksFiles]
CHDRT64.sys=222
UIU64a.exe=222
UCI64A52.dll=222
CX64AQ17.dll=222
VoipUpdate.ini=222

[Manufacturer]
Conexant = Conexant, NTamd64.6.0
 
;============================================================================

[ControlFlags]
ExcludeFromSelect = *
[Conexant.NTamd64.6.0]
%HdAudioFunctionDriver.Pebble5071.DeviceDesc% = HdAudModel.SHINMV, HDAUDIO\FUNC_01&VEN_14F1&DEV_5069&SUBSYS_17AA21A4
%HdAudioFunctionDriver.Pebble5071.DeviceDesc% = HdAudModel.NZMI1, HDAUDIO\FUNC_01&VEN_14F1&DEV_5069&SUBSYS_17AA214C
%HdAudioFunctionDriver.Pebble5071.DeviceDesc% = HdAudModel.NICO3, HDAUDIO\FUNC_01&VEN_14F1&DEV_5069&SUBSYS_17AA2151
%HdAudioFunctionDriver.Pebble5071.DeviceDesc% = HdAudModel.MOCA3, HDAUDIO\FUNC_01&VEN_14F1&DEV_5069&SUBSYS_17AA2155
%HdAudioFunctionDriver.Pebble5071.DeviceDesc% = HdAudModel.PCAN3, HDAUDIO\FUNC_01&VEN_14F1&DEV_5069&SUBSYS_17AA2156
%HdAudioFunctionDriver.Pebble5071.DeviceDesc% = HdAudModel.CRML3, HDAUDIO\FUNC_01&VEN_14F1&DEV_5069&SUBSYS_17AA2157
%HdAudioFunctionDriver.Pebble5071.DeviceDesc% = HdAudModel.KNDO, HDAUDIO\FUNC_01&VEN_14F1&DEV_5069&SUBSYS_17AA218B
 
[HdAudModel.SHINMV.NT]
Include=ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration,mssysfx.CopyFilesAndRegister
CopyFiles = HdAudModel.Copyfiles, Uninstall.CopyFiles, SfxFx.CopyList
AddReg    = HdAudModel.BF.AddReg, Oem.SHINMV.AddReg, AECDRC.AddReg, LnVoIP.AddReg, SoftEQ.SHINMV.AddReg, EffectsEQ.AddReg, HdAudInit.AddReg, Uninstall.AddReg, Misc.AddReg
AddProperty = HdAudBranding.AddProperty
RegisterDlls=SfxFx.RegisterDlls
 
[HdAudModel.NZMI1.NT]
Include=ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration,mssysfx.CopyFilesAndRegister
CopyFiles = HdAudModel.Copyfiles, Uninstall.CopyFiles, SfxFx.CopyList
AddReg    = HdAudModel.BF.AddReg, Oem.NZMI1.AddReg, AECDRC.AddReg, LnVoIP.AddReg, SoftEQ.NZMI1.AddReg, EffectsEQ.AddReg, HdAudInit.AddReg, Uninstall.AddReg, Misc.AddReg
AddProperty = HdAudBranding.AddProperty
 
RegisterDlls=SfxFx.RegisterDlls
 
[HdAudModel.NICO3.NT]
Include=ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration,mssysfx.CopyFilesAndRegister
CopyFiles = HdAudModel.Copyfiles, Uninstall.CopyFiles, SfxFx.CopyList
AddReg    = HdAudModel.NoBF.AddReg, Oem.NICO3.AddReg, AECDRC.AddReg, LnVoIP.AddReg, SoftEQ.NICO3.AddReg, EffectsEQ.AddReg, HdAudInit.AddReg, Uninstall.AddReg, Misc.AddReg
AddProperty = HdAudBranding.AddProperty
RegisterDlls=SfxFx.RegisterDlls
 
[HdAudModel.MOCA3.NT]
Include=ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration,mssysfx.CopyFilesAndRegister
CopyFiles = HdAudModel.Copyfiles, Uninstall.CopyFiles, SfxFx.CopyList
AddReg    = HdAudModel.NoBF.AddReg, Oem.MOCA3.AddReg, AECDRC.AddReg, LnVoIP.AddReg, SoftEQ.MOCA3.AddReg, EffectsEQ.AddReg, HdAudInit.AddReg, Uninstall.AddReg, Misc.AddReg
AddProperty = HdAudBranding.AddProperty
 
RegisterDlls=SfxFx.RegisterDlls
 
[HdAudModel.PCAN3.NT]
Include=ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration,mssysfx.CopyFilesAndRegister
CopyFiles = HdAudModel.Copyfiles, Uninstall.CopyFiles, SfxFx.CopyList
AddReg    = HdAudModel.NoBF.AddReg, Oem.PCAN3.AddReg, AECDRC.AddReg, LnVoIP.AddReg, SoftEQ.PCAN3.AddReg, EffectsEQ.AddReg, HdAudInit.PCAN3.AddReg, Uninstall.AddReg, Misc.AddReg
AddProperty = HdAudBranding.AddProperty
RegisterDlls=SfxFx.RegisterDlls
 
[HdAudModel.CRML3.NT]
Include=ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration,mssysfx.CopyFilesAndRegister
CopyFiles = HdAudModel.Copyfiles, Uninstall.CopyFiles, SfxFx.CopyList
AddReg    = HdAudModel.CRML3.BF.AddReg, Oem.CRML3.AddReg, AECDRC.AddReg, LnVoIP.AddReg, SoftEQ.CRML3.AddReg, EffectsEQ.AddReg, HdAudInit.AddReg, Uninstall.AddReg, Misc.AddReg
AddProperty = HdAudBranding.AddProperty
 
RegisterDlls=SfxFx.RegisterDlls
 
[HdAudModel.KNDO.NT]
Include=ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration,mssysfx.CopyFilesAndRegister
CopyFiles = HdAudModel.Copyfiles, Uninstall.CopyFiles, SfxFx.CopyList
AddReg    = HdAudModel.KNDO.BF.AddReg, Oem.KNDO.AddReg, AECDRC.AddReg, LnVoIP.AddReg, SoftEQ.KNDO.AddReg, EffectsEQ.AddReg, HdAudInit.AddReg, Uninstall.AddReg, Misc.AddReg
AddProperty = HdAudBranding.AddProperty
RegisterDlls=SfxFx.RegisterDlls
 
[HdAudModel.SHINMV.NT.HW]
AddReg = HdAudSecurity.AddReg

[HdAudModel.NZMI1.NT.HW]
AddReg = HdAudSecurity.AddReg
 
[HdAudModel.NICO3.NT.HW]
AddReg = HdAudSecurity.AddReg
 
[HdAudModel.MOCA3.NT.HW]
AddReg = HdAudSecurity.AddReg
 
[HdAudModel.PCAN3.NT.HW]
AddReg = HdAudSecurity.AddReg
 
[HdAudModel.CRML3.NT.HW]
AddReg = HdAudSecurity.AddReg
 
[HdAudModel.KNDO.NT.HW]
AddReg = HdAudSecurity.AddReg
 
[HdAudModel.SHINMV.NT.Services]
AddService=CnxtHdAudService, 0x00000002, HdAud_Service_Install

[HdAudModel.NZMI1.NT.Services]
AddService=CnxtHdAudService, 0x00000002, HdAud_Service_Install
 
[HdAudModel.NICO3.NT.Services]
AddService=CnxtHdAudService, 0x00000002, HdAud_Service_Install
 
[HdAudModel.MOCA3.NT.Services]
AddService=CnxtHdAudService, 0x00000002, HdAud_Service_Install
 
[HdAudModel.PCAN3.NT.Services]
AddService=CnxtHdAudService, 0x00000002, HdAud_Service_Install
 
[HdAudModel.CRML3.NT.Services]
AddService=CnxtHdAudService, 0x00000002, HdAud_Service_Install
 
[HdAudModel.KNDO.NT.Services]
AddService=CnxtHdAudService, 0x00000002, HdAud_Service_Install
 
[HdAud_Service_Install]
DisplayName   = %UAAFunctionDriverForHdAudio.SvcDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\CHDRT64.sys

[Uninstall.CopyFiles]
UIU64a.exe
 
[HdAudModel.SHINMV.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[HdAudModel.NZMI1.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles
 
[HdAudModel.NICO3.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles
 
[HdAudModel.MOCA3.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles
 
[HdAudModel.PCAN3.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles
 
[HdAudModel.CRML3.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles
 
[HdAudModel.KNDO.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles
 
[CoInstaller_CopyFiles]
UCI64A52.dll
VoipUpdate.ini

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000,"UCI64A52.dll,CAUDCoInstaller"

[Uninstall.AddReg]
; Files to Delete...
HKLM, SOFTWARE\%CompanyName%\%ProductName%\Files\SYS,CHDRT64.sys,,"CHDRT64.sys"
HKLM, SOFTWARE\%CompanyName%\%ProductName%\RegKeys,"Software\Microsoft\Windows\CurrentVersion\Uninstall",,%UIPATH%
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%UIPATH%",DisplayName,,%HDAudioOEMFriendlyName%
HKLM, SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%UIPATH%, DisplayVersion,,%VersionInfo%
HKLM, SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%UIPATH%, VersionMajor,,4
HKLM, SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%UIPATH%, VersionMinor,,95
HKLM, SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%UIPATH%, Publisher,,%CompanyName%
HKLM, SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%UIPATH%, DisplayIcon,,%16422%\CONEXANT\%UIPATH%\UIU64a.exe
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%UIPATH%",UninstallString,,%16422%\CONEXANT\%UIPATH%\UIU64a.exe -U -ITPUNPEBy.INF

[HdAudModel.Copyfiles]
CHDRT64.sys
[HdAudBranding.AddProperty]
DeviceVendorWebSite,,,,"http://www.conexant.com"
 
[HdAudInit.AddReg]
;; Sample Section to Illustrate the format for Initialization verbs.
;; Uncomment and add appropriate verbs as needed.
;; Note that the top nibble of the verb (Codec Address) must be '0'.
HKR,InitVerbs,NumVerbs,0x00010001, 0x00000004 ; Example: Number of verbs in the init section
HKR,InitVerbs,0000, 0x00010001, 0x02529088  ; Sets HPF to 120Hz
HKR,InitVerbs,0001, 0x00010001, 0x02539057  ; Sets TP to 100
HKR,InitVerbs,0002, 0x00010001, 0x0252F000  ; Disable Debounce
HKR,InitVerbs,0003, 0x00010001, 0x01370A00  ; Disable Beep Generator  
;HKR,InitVerbs,0000,    0x00010001, 0x01E71C01 ; Sets first byte of pin config info
;HKR,InitVerbs,0001,    0x00010001, 0x01E71D44 ; Sets second byte of pin config info
;HKR,InitVerbs,0002,    0x00010001, 0x01E71E21 ; Sets third byte of pin config info
;HKR,InitVerbs,0003,    0x00010001, 0x01E71F00 ; Sets fourth byte of pin config info

[HdAudInit.PCAN3.AddReg]
;; Sample Section to Illustrate the format for Initialization verbs.
;; Uncomment and add appropriate verbs as needed.
;; Note that the top nibble of the verb (Codec Address) must be '0'.
HKR,InitVerbs,NumVerbs,0x00010001, 0x00000005 ; Example: Number of verbs in the init section
HKR,InitVerbs,0000, 0x00010001, 0x02527010  ; Sets Pecan to Mono spkr
HKR,InitVerbs,0001, 0x00010001, 0x02529088  ; Sets HPF to 120Hz
HKR,InitVerbs,0002, 0x00010001, 0x02539057  ; Sets TP to 100
HKR,InitVerbs,0003, 0x00010001, 0x0252F000  ; Disable Debounce
HKR,InitVerbs,0004, 0x00010001, 0x01370A00  ; Disable Beep Generator  
 
[HdAudModel.BF.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,CHDRT64.sys
HKR,,SSFriendlyName,,%RearLineOutWaveDeviceName%
HKR,,CompanyName,,%CompanyName%
HKR,,ProductName,,%ProductName%

HKR,Drivers,SubClasses,,"wave,midi,mixer,aux"

HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\aux\wdmaud.drv,Driver,,wdmaud.drv

HKR,Drivers\wave\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\midi\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\mixer\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\aux\wdmaud.drv,Description,,%HdAudioDeviceDescription%

;;disable SetupPreferredAudioDevices, this will pick up SPDIF as default
;;HKR,,SetupPreferredAudioDevices,3,01,00,00,00
HKR,,DisableSetupDiChangeState,1,00,00,00,00 ; Set to 01,00,00,00 to disable proppage restarting of driver on policy change
; Driver global settings
;;HKR,GlobalSettings,DcOffsetWorkaround,1,01,00,00,00 ; Applies workaround for recording DC offset issue
HKR,GlobalSettings,ResetAudioFgOnStart,1,00,00,00,00 ; Enables resetting of audio FG on driver start
HKR,GlobalSettings,SysAudioTopoMiniportWorkaround,1,01,00,00,00 ; Enables holding ref on topo port & miniport when device is uninstantiated

HKR,GlobalSettings,ValidateCodecWrites,1,00,00,00,00 ; Enables readback of writes to codec registers
HKR,GlobalSettings,SendFakePcxCfgDefVerbs,1,00,00,00,00 ; Enables sending fake pin config default table
HKR,GlobalSettings,SpdifOutputEchosRearRenderWhenNoAc3,1,00,00,00,00 ; Slaves rear panel front channels to SPDIF
HKR,GlobalSettings,HpShutsOffRearSpeaker,1,00,00,00,00 ; Headphone does not mute rear speakers
HKR,GlobalSettings,HpMode,1,01,00,00,00 ; Headphone is slaved to rear panel front channels
HKR,GlobalSettings,EnableDynamicDevices,1,00,00,00,00 ; Headphone will come and go dynamically.
HKR,GlobalSettings,SetSpdifVCfg,1,01,00,00,00 ;  VCfg bit will be set on SPDIF out
HKR,GlobalSettings,MaxLatencyInMS,1,FF,00,00,00 ; Max Latency Supported in MS
HKR,GlobalSettings,MaxAc3LatencyInMS,1,19,00,00,00 ; Max Latency for AC3 Streams in MS: 0x19 is 25MS
HKR,GlobalSettings,StartDelayInMS,1,0A,00,00,00 ; Stream Startup Delay in MS
HKR,GlobalSettings,MaxReadAheadInMS,1,0A,00,00,00 ; Max amount of data to read ahead in a directsound buffer
HKR,GlobalSettings,MaxKmixerReadAheadInMS,1,28,00,00,00 ; Max amount of data to read ahead in a Kmixer buffer
HKR,GlobalSettings,BeamWidth,1,14,00,46,00 ;; Beam Width and Mic Array Seperation
HKR,GlobalSettings,MicNrAgressivenessLevel,1,04,00,00,00 ; Mic NR Agressiveness
HKR,GlobalSettings,SpkrNrAgressivenessLevel,1,00,00,00,00 ; Speaker NR agressiveness
HKR,GlobalSettings,ShutdownDelay,1,C8,00,00,00 ; Power Down and Suspend Delay in ms
 
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates44100,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates48000,1,01,00,00,00 ; By default, only one supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates96000,1,00,00,00,00 ; By default, not supported
 
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths16,1,01,00,00,00 ; By default, only one supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths20,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths24,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths32,1,00,00,00,00 ; By default, not supported
 
HKR,GlobalSettings\\SpdifIn,SpdifInputBitDepth,1,00,00,00,00 ; By default, 16 bit digital capture
HKR,GlobalSettings\\SpdifIn,SpdifInputSampleRate,1,01,00,00,00; By default, 48KHz digital capture
 
HKR,PowerSettings,ConservationIdleTime,1,00,00,00,00
HKR,PowerSettings,PerformanceIdleTime,1,00,00,00,00
HKR,PowerSettings,IdlePowerState,1,00,00,00,00
 
;AmpControl
HKR,Settings\AmpControl,AmpControlOptions,1,E9,E8,00,01
HKR,Settings\AmpControl,AmpControlPortOptions,1,64,00,00,00
 
[HdAudModel.KNDO.BF.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,CHDRT64.sys
HKR,,SSFriendlyName,,%RearLineOutWaveDeviceName%
HKR,,CompanyName,,%CompanyName%
HKR,,ProductName,,%ProductName%
 
HKR,Drivers,SubClasses,,"wave,midi,mixer,aux"
 
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\aux\wdmaud.drv,Driver,,wdmaud.drv
 
HKR,Drivers\wave\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\midi\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\mixer\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\aux\wdmaud.drv,Description,,%HdAudioDeviceDescription%
 
;;disable SetupPreferredAudioDevices, this will pick up SPDIF as default
;;HKR,,SetupPreferredAudioDevices,3,01,00,00,00
HKR,,DisableSetupDiChangeState,1,00,00,00,00 ; Set to 01,00,00,00 to disable proppage restarting of driver on policy change
; Driver global settings
;;HKR,GlobalSettings,DcOffsetWorkaround,1,01,00,00,00 ; Applies workaround for recording DC offset issue
HKR,GlobalSettings,ResetAudioFgOnStart,1,00,00,00,00 ; Enables resetting of audio FG on driver start
HKR,GlobalSettings,SysAudioTopoMiniportWorkaround,1,01,00,00,00 ; Enables holding ref on topo port & miniport when device is uninstantiated
 
HKR,GlobalSettings,ValidateCodecWrites,1,00,00,00,00 ; Enables readback of writes to codec registers
HKR,GlobalSettings,SendFakePcxCfgDefVerbs,1,00,00,00,00 ; Enables sending fake pin config default table
HKR,GlobalSettings,SpdifOutputEchosRearRenderWhenNoAc3,1,00,00,00,00 ; Slaves rear panel front channels to SPDIF
HKR,GlobalSettings,HpShutsOffRearSpeaker,1,00,00,00,00 ; Headphone does not mute rear speakers
HKR,GlobalSettings,HpMode,1,01,00,00,00 ; Headphone is slaved to rear panel front channels
HKR,GlobalSettings,EnableDynamicDevices,1,00,00,00,00 ; Headphone will come and go dynamically.
HKR,GlobalSettings,SetSpdifVCfg,1,01,00,00,00 ;  VCfg bit will be set on SPDIF out
HKR,GlobalSettings,MaxLatencyInMS,1,FF,00,00,00 ; Max Latency Supported in MS
HKR,GlobalSettings,MaxAc3LatencyInMS,1,19,00,00,00 ; Max Latency for AC3 Streams in MS: 0x19 is 25MS
HKR,GlobalSettings,StartDelayInMS,1,0A,00,00,00 ; Stream Startup Delay in MS
HKR,GlobalSettings,MaxReadAheadInMS,1,0A,00,00,00 ; Max amount of data to read ahead in a directsound buffer
HKR,GlobalSettings,MaxKmixerReadAheadInMS,1,28,00,00,00 ; Max amount of data to read ahead in a Kmixer buffer
HKR,GlobalSettings,BeamWidth,1,14,00,64,00 ;; Beam Width and Mic Array Seperation
HKR,GlobalSettings,MicNrAgressivenessLevel,1,04,00,00,00 ; Mic NR Agressiveness
HKR,GlobalSettings,SpkrNrAgressivenessLevel,1,00,00,00,00 ; Speaker NR agressiveness
HKR,GlobalSettings,ShutdownDelay,1,C8,00,00,00 ; Power Down and Suspend Delay in ms
 
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates44100,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates48000,1,01,00,00,00 ; By default, only one supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates96000,1,00,00,00,00 ; By default, not supported
 
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths16,1,01,00,00,00 ; By default, only one supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths20,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths24,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths32,1,00,00,00,00 ; By default, not supported
 
HKR,GlobalSettings\\SpdifIn,SpdifInputBitDepth,1,00,00,00,00 ; By default, 16 bit digital capture
HKR,GlobalSettings\\SpdifIn,SpdifInputSampleRate,1,01,00,00,00; By default, 48KHz digital capture
 
HKR,PowerSettings,ConservationIdleTime,1,00,00,00,00
HKR,PowerSettings,PerformanceIdleTime,1,00,00,00,00
HKR,PowerSettings,IdlePowerState,1,00,00,00,00
 
;AmpControl
HKR,Settings\AmpControl,AmpControlOptions,1,E9,E8,00,01
HKR,Settings\AmpControl,AmpControlPortOptions,1,64,00,00,00
 
[HdAudModel.CRML3.BF.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,CHDRT64.sys
HKR,,SSFriendlyName,,%RearLineOutWaveDeviceName%
HKR,,CompanyName,,%CompanyName%
HKR,,ProductName,,%ProductName%
 
HKR,Drivers,SubClasses,,"wave,midi,mixer,aux"
 
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\aux\wdmaud.drv,Driver,,wdmaud.drv
 
HKR,Drivers\wave\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\midi\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\mixer\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\aux\wdmaud.drv,Description,,%HdAudioDeviceDescription%
 
;;disable SetupPreferredAudioDevices, this will pick up SPDIF as default
;;HKR,,SetupPreferredAudioDevices,3,01,00,00,00
HKR,,DisableSetupDiChangeState,1,00,00,00,00 ; Set to 01,00,00,00 to disable proppage restarting of driver on policy change
; Driver global settings
;;HKR,GlobalSettings,DcOffsetWorkaround,1,01,00,00,00 ; Applies workaround for recording DC offset issue
HKR,GlobalSettings,ResetAudioFgOnStart,1,00,00,00,00 ; Enables resetting of audio FG on driver start
HKR,GlobalSettings,SysAudioTopoMiniportWorkaround,1,01,00,00,00 ; Enables holding ref on topo port & miniport when device is uninstantiated
 
HKR,GlobalSettings,ValidateCodecWrites,1,00,00,00,00 ; Enables readback of writes to codec registers
HKR,GlobalSettings,SendFakePcxCfgDefVerbs,1,00,00,00,00 ; Enables sending fake pin config default table
HKR,GlobalSettings,SpdifOutputEchosRearRenderWhenNoAc3,1,00,00,00,00 ; Slaves rear panel front channels to SPDIF
HKR,GlobalSettings,HpShutsOffRearSpeaker,1,00,00,00,00 ; Headphone does not mute rear speakers
HKR,GlobalSettings,HpMode,1,01,00,00,00 ; Headphone is slaved to rear panel front channels
HKR,GlobalSettings,EnableDynamicDevices,1,00,00,00,00 ; Headphone will come and go dynamically.
HKR,GlobalSettings,SetSpdifVCfg,1,01,00,00,00 ;  VCfg bit will be set on SPDIF out
HKR,GlobalSettings,MaxLatencyInMS,1,FF,00,00,00 ; Max Latency Supported in MS
HKR,GlobalSettings,MaxAc3LatencyInMS,1,19,00,00,00 ; Max Latency for AC3 Streams in MS: 0x19 is 25MS
HKR,GlobalSettings,StartDelayInMS,1,0A,00,00,00 ; Stream Startup Delay in MS
HKR,GlobalSettings,MaxReadAheadInMS,1,0A,00,00,00 ; Max amount of data to read ahead in a directsound buffer
HKR,GlobalSettings,MaxKmixerReadAheadInMS,1,28,00,00,00 ; Max amount of data to read ahead in a Kmixer buffer
HKR,GlobalSettings,BeamWidth,1,14,00,55,00 ;; Beam Width and Mic Array Seperation
HKR,GlobalSettings,MicNrAgressivenessLevel,1,04,00,00,00 ; Mic NR Agressiveness
HKR,GlobalSettings,SpkrNrAgressivenessLevel,1,00,00,00,00 ; Speaker NR agressiveness
HKR,GlobalSettings,ShutdownDelay,1,C8,00,00,00 ; Power Down and Suspend Delay in ms
 
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates44100,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates48000,1,01,00,00,00 ; By default, only one supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates96000,1,00,00,00,00 ; By default, not supported
 
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths16,1,01,00,00,00 ; By default, only one supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths20,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths24,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths32,1,00,00,00,00 ; By default, not supported
 
HKR,GlobalSettings\\SpdifIn,SpdifInputBitDepth,1,00,00,00,00 ; By default, 16 bit digital capture
HKR,GlobalSettings\\SpdifIn,SpdifInputSampleRate,1,01,00,00,00; By default, 48KHz digital capture
 
HKR,PowerSettings,ConservationIdleTime,1,00,00,00,00
HKR,PowerSettings,PerformanceIdleTime,1,00,00,00,00
HKR,PowerSettings,IdlePowerState,1,00,00,00,00
 
;AmpControl
HKR,Settings\AmpControl,AmpControlOptions,1,E9,E8,00,01
HKR,Settings\AmpControl,AmpControlPortOptions,1,64,00,00,00
 
[HdAudModel.NoBF.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,CHDRT64.sys
HKR,,SSFriendlyName,,%RearLineOutWaveDeviceName%
HKR,,CompanyName,,%CompanyName%
HKR,,ProductName,,%ProductName%
 
HKR,Drivers,SubClasses,,"wave,midi,mixer,aux"
 
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\aux\wdmaud.drv,Driver,,wdmaud.drv
 
HKR,Drivers\wave\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\midi\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\mixer\wdmaud.drv,Description,,%HdAudioDeviceDescription%
HKR,Drivers\aux\wdmaud.drv,Description,,%HdAudioDeviceDescription%
 
;;disable SetupPreferredAudioDevices, this will pick up SPDIF as default
;;HKR,,SetupPreferredAudioDevices,3,01,00,00,00
HKR,,DisableSetupDiChangeState,1,00,00,00,00 ; Set to 01,00,00,00 to disable proppage restarting of driver on policy change
; Driver global settings
;;HKR,GlobalSettings,DcOffsetWorkaround,1,01,00,00,00 ; Applies workaround for recording DC offset issue
HKR,GlobalSettings,ResetAudioFgOnStart,1,00,00,00,00 ; Enables resetting of audio FG on driver start
HKR,GlobalSettings,SysAudioTopoMiniportWorkaround,1,01,00,00,00 ; Enables holding ref on topo port & miniport when device is uninstantiated
 
HKR,GlobalSettings,ValidateCodecWrites,1,00,00,00,00 ; Enables readback of writes to codec registers
HKR,GlobalSettings,SendFakePcxCfgDefVerbs,1,00,00,00,00 ; Enables sending fake pin config default table
HKR,GlobalSettings,SpdifOutputEchosRearRenderWhenNoAc3,1,00,00,00,00 ; Slaves rear panel front channels to SPDIF
HKR,GlobalSettings,HpShutsOffRearSpeaker,1,00,00,00,00 ; Headphone does not mute rear speakers
HKR,GlobalSettings,HpMode,1,01,00,00,00 ; Headphone is slaved to rear panel front channels
HKR,GlobalSettings,EnableDynamicDevices,1,00,00,00,00 ; Headphone will come and go dynamically.
HKR,GlobalSettings,SetSpdifVCfg,1,01,00,00,00 ;  VCfg bit will be set on SPDIF out
HKR,GlobalSettings,MaxLatencyInMS,1,FF,00,00,00 ; Max Latency Supported in MS
HKR,GlobalSettings,MaxAc3LatencyInMS,1,19,00,00,00 ; Max Latency for AC3 Streams in MS: 0x19 is 25MS
HKR,GlobalSettings,StartDelayInMS,1,0A,00,00,00 ; Stream Startup Delay in MS
HKR,GlobalSettings,MaxReadAheadInMS,1,0A,00,00,00 ; Max amount of data to read ahead in a directsound buffer
HKR,GlobalSettings,MaxKmixerReadAheadInMS,1,28,00,00,00 ; Max amount of data to read ahead in a Kmixer buffer
HKR,GlobalSettings,BeamWidth,1,14,00,7f,00 ;; Beam Width and Mic Array Seperation
HKR,GlobalSettings,MicNrAgressivenessLevel,1,04,00,00,00 ; Mic NR Agressiveness
HKR,GlobalSettings,SpkrNrAgressivenessLevel,1,00,00,00,00 ; Speaker NR agressiveness
HKR,GlobalSettings,ShutdownDelay,1,C8,00,00,00 ; Power Down and Suspend Delay in ms
 
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates44100,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates48000,1,01,00,00,00 ; By default, only one supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedSampleRates96000,1,00,00,00,00 ; By default, not supported
 
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths16,1,01,00,00,00 ; By default, only one supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths20,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths24,1,00,00,00,00 ; By default, not supported
HKR,GlobalSettings\\SpdifOut,ExternalSpdifReceiverSupportedBitDepths32,1,00,00,00,00 ; By default, not supported
 
HKR,GlobalSettings\\SpdifIn,SpdifInputBitDepth,1,00,00,00,00 ; By default, 16 bit digital capture
HKR,GlobalSettings\\SpdifIn,SpdifInputSampleRate,1,01,00,00,00; By default, 48KHz digital capture
 
HKR,PowerSettings,ConservationIdleTime,1,00,00,00,00
HKR,PowerSettings,PerformanceIdleTime,1,00,00,00,00
HKR,PowerSettings,IdlePowerState,1,00,00,00,00
 
;AmpControl
HKR,Settings\AmpControl,AmpControlOptions,1,E9,E8,00,01
HKR,Settings\AmpControl,AmpControlPortOptions,1,64,00,00,00
 
[Misc.AddReg]
HKLM,SYSTEM\CurrentControlSet\Control\Conexant\LvlRelAdjust,NightModeGainBoost,0x10001,0x00090000
 
[Oem.SHINMV.AddReg]
HKR,Settings\OEM,Flags,1,72,38,00,5A
HKR,Settings\OEM,Flags2,1,A2,31,B4,7F
HKR,Settings\OEM,Flags3,1,80,08,02,10
HKR,Settings\OEM,Flags4,1,80,78,10,00
HKR,Settings\OEM,Flags5,1,00,04,41,00
HKR,Settings\OEM,PortsCap,1,00,27,27,00
HKR,Settings\OEM,EqProfile,1,01,00,00,00
HKR,Settings\OEM,SmartAudioSettings,1,D8,11,00,00
HKR,Settings\OEM,NumOfSoftStream,1,01,01,00,00
HKR,Settings\OEM,DefaultGain,1,13,00,2B,14,00,00,00,00
HKR,Settings\OEM,DefaultAECMicLowLevel,1,00,00,00,00
HKR,Settings\OEM,DefaultAECMicHighLevel,1,00,00,18,00
HKR,Settings\OEM,SASpatializerPhantomSPSpread,1,40,00,00,00
HKR,Settings\OEM,SASpatializerImmersionSpread,1,40,00,00,00
HKR,Settings\OEM,TestRegBypassIndex,1,1A,00,00,00,00,00,00,00
HKR,Settings\OEM\DefaultJack,Wid19,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1A,1,0a,00,00,02 
HKR,Settings\OEM\DefaultJack,Wid1B,1,0a,00,00,01 
HKR,Settings\OEM\DefaultJack,Wid1C,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1D,1,01,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1E,1,0a,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1F,1,01,00,01,00
HKR,Settings\OEM\DefaultJack,Wid23,1,0a,00,01,00 
HKR,Settings\OEM\DefaultJack,Wid27,1,0a,00,00,00 
HKR,Settings\OEM\InitialSliderPosition,InitialMasterPlaybackPos,1,C9,7A,F8,FF
HKR,Settings\OEM\InitialSliderPosition,InitialLineInPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialWaveOutMixCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxCapturePos,1,C9,FA,0E,00
HKR,Settings\OEM\InitialSliderPosition,InitialLineInCapturePos,1,C9,7A,10,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicCapturePos,1,00,00,06,00
HKR,Settings\OEM\InitialSliderPosition,InitialCDCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicBoostCapturePos,1,00,00,24,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxMicBoostCapturePos,1,00,00,1E,00
 
;default Min for Pebble is 0xffb60000(-74dB), default Max for Pebble is 0x60000(+6dB)
;default Min for Venice is 0x00000000(0dB), default Max for Venice is 0x228000(+34.5dB)
;default Min for Waikiki is 0x00000000(0dB), default Max for Waikiki is 0x150000(+21dB)
;note 0x10000=1dB, 0x8000=0.5dB
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMax,1,00,00,06,00 
HKR,Settings\OEM\MicInRange,DigiMicBoostOffset,1,00,00,f8,ff 
HKR,Settings\OEM\MicInRange,IntMicDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortBDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortCDefaultBoostGainStep,1,02,00,00,00
 
HKR,Settings\OEM\MicInRange,PortAMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortAMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortBMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBBoostOffset,1,00,00,10,00
HKR,Settings\OEM\MicInRange,PortCMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortCMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortCBoostOffset,1,00,00,10,00	
HKR,Settings\OEM\MicInRange,PortFMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMax,1,00,00,06,00	
 
HKR,Settings\OEM\LineInRange,PortALineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortALineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortBLineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortBLineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortCLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortCLineInMax,1,00,00,06,00	
HKR,Settings\OEM\LineInRange,PortFLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortFLineInMax,1,00,00,06,00	
 
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMin,1,00,00,00,00
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMax,1,00,80,22,00
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMin,1,00,00,A0,FF
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMax,1,00,00,0C,00
 
;    64 = 100% of the volume possible,etc...
;    32 = 50% of the volume possible,etc...
HKR,Settings\OEM\FlexSettings,Flex_MasterPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDPlaybackVolume,0x00000001,2D,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_WaveOutMixCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_AuxCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDCaptureVolume,0x00000001,64,00,00,00
 
; PortRules changed to ULONGLONG, 64bits
HKR,Settings\PortRules,NumOfRules,1,07,00,00,00
HKR,Settings\PortRules,PortRules,1,\
11,62,6F,6F,62,6F,6F,51,\
10,52,6F,6F,72,6F,6F,71,\
10,52,6F,6F,62,6F,6F,71,\
10,62,6F,6F,52,6F,6F,71,\
90,52,4F,4F,52,4F,4F,71,\
90,52,4F,4F,42,4F,4F,51,\
90,42,4F,4F,52,4F,4F,51
 
HKR,Settings\MicInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\MicInPortRules,PortRules,1,\
10,4F,3A,4F,4F,4F,0A,4F,\
10,4F,0A,4F,4F,4F,3A,4F
 
HKR,Settings\LineInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\LineInPortRules,PortRules,1,\
10,4F,4F,08,4F,4F,4F,4F,\
10,4F,4F,58,4F,4F,4F,4F
 
;PEBBLE port configuration settings
HKR,Settings\PortConfig\ClassicModeCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,NumOfPorts,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialSliderPos,1,00,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1,1,1e,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2,1,23,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3,1,1a,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4,1,1b,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1Priority,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2Priority,1,03,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3Priority,1,02,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1,1,1b,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection2,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialSliderPos,1,00,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1,1,1a,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1Priority,1,01,00,00,00
 
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,NumOfPorts,1,01,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1,1,24,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1,1,23,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1Priority,1,02,00,00,00
 
[Oem.NZMI1.AddReg]
HKR,Settings\OEM,Flags,1,72,38,00,5A
HKR,Settings\OEM,Flags2,1,A2,31,B4,7F
HKR,Settings\OEM,Flags3,1,80,08,02,10
HKR,Settings\OEM,Flags4,1,80,78,10,00
HKR,Settings\OEM,Flags5,1,00,04,41,00
HKR,Settings\OEM,PortsCap,1,00,27,27,00
HKR,Settings\OEM,EqProfile,1,01,00,00,00
HKR,Settings\OEM,SmartAudioSettings,1,D8,11,00,00
HKR,Settings\OEM,NumOfSoftStream,1,01,01,00,00
HKR,Settings\OEM,DefaultGain,1,13,00,2B,14,00,00,00,00
HKR,Settings\OEM,DefaultAECMicLowLevel,1,00,00,00,00
HKR,Settings\OEM,DefaultAECMicHighLevel,1,00,00,18,00
HKR,Settings\OEM,SASpatializerPhantomSPSpread,1,40,00,00,00
HKR,Settings\OEM,SASpatializerImmersionSpread,1,40,00,00,00
HKR,Settings\OEM,TestRegBypassIndex,1,1A,00,00,00,00,00,00,00
HKR,Settings\OEM\DefaultJack,Wid19,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1A,1,0a,00,00,02 
HKR,Settings\OEM\DefaultJack,Wid1B,1,0a,00,00,01 
HKR,Settings\OEM\DefaultJack,Wid1C,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1D,1,01,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1E,1,0a,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1F,1,01,00,01,00
HKR,Settings\OEM\DefaultJack,Wid23,1,0a,00,01,00 
HKR,Settings\OEM\DefaultJack,Wid27,1,0a,00,00,00 
HKR,Settings\OEM\InitialSliderPosition,InitialMasterPlaybackPos,1,C9,7A,F8,FF
HKR,Settings\OEM\InitialSliderPosition,InitialLineInPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialWaveOutMixCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxCapturePos,1,C9,FA,0E,00
HKR,Settings\OEM\InitialSliderPosition,InitialLineInCapturePos,1,C9,7A,10,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicCapturePos,1,00,00,06,00
HKR,Settings\OEM\InitialSliderPosition,InitialCDCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicBoostCapturePos,1,00,00,24,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxMicBoostCapturePos,1,00,00,1E,00
 
;default Min for Pebble is 0xffb60000(-74dB), default Max for Pebble is 0x60000(+6dB)
;default Min for Venice is 0x00000000(0dB), default Max for Venice is 0x228000(+34.5dB)
;default Min for Waikiki is 0x00000000(0dB), default Max for Waikiki is 0x150000(+21dB)
;note 0x10000=1dB, 0x8000=0.5dB
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMax,1,00,00,06,00 
HKR,Settings\OEM\MicInRange,DigiMicBoostOffset,1,00,00,EC,FF
HKR,Settings\OEM\MicInRange,IntMicDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortBDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortCDefaultBoostGainStep,1,02,00,00,00
 
HKR,Settings\OEM\MicInRange,PortAMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortAMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortBMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBBoostOffset,1,00,00,02,00
HKR,Settings\OEM\MicInRange,PortCMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortCMicInMax,1,00,00,16,00	
HKR,Settings\OEM\MicInRange,PortCBoostOffset,1,00,00,F8,FF
HKR,Settings\OEM\MicInRange,PortFMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMax,1,00,00,06,00	
 
HKR,Settings\OEM\LineInRange,PortALineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortALineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortBLineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortBLineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortCLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortCLineInMax,1,00,00,06,00	
HKR,Settings\OEM\LineInRange,PortFLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortFLineInMax,1,00,00,06,00	
 
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMin,1,00,00,00,00
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMax,1,00,80,22,00
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMin,1,00,00,A0,FF
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMax,1,00,00,0C,00
 
;    64 = 100% of the volume possible,etc...
;    32 = 50% of the volume possible,etc...
HKR,Settings\OEM\FlexSettings,Flex_MasterPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDPlaybackVolume,0x00000001,2D,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_WaveOutMixCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_AuxCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDCaptureVolume,0x00000001,64,00,00,00
 
; PortRules changed to ULONGLONG, 64bits
HKR,Settings\PortRules,NumOfRules,1,07,00,00,00
HKR,Settings\PortRules,PortRules,1,\
11,62,6F,6F,62,6F,6F,51,\
10,52,6F,6F,72,6F,6F,71,\
10,52,6F,6F,62,6F,6F,71,\
10,62,6F,6F,52,6F,6F,71,\
90,52,4F,4F,52,4F,4F,71,\
90,52,4F,4F,42,4F,4F,51,\
90,42,4F,4F,52,4F,4F,51
 
HKR,Settings\MicInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\MicInPortRules,PortRules,1,\
10,4F,3A,4F,4F,4F,0A,4F,\
10,4F,0A,4F,4F,4F,3A,4F
 
HKR,Settings\LineInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\LineInPortRules,PortRules,1,\
10,4F,4F,08,4F,4F,4F,4F,\
10,4F,4F,58,4F,4F,4F,4F
 
;PEBBLE port configuration settings
HKR,Settings\PortConfig\ClassicModeCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,NumOfPorts,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1,1,1e,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2,1,23,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3,1,1a,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4,1,1b,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1Priority,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2Priority,1,03,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3Priority,1,02,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1,1,1b,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection2,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1,1,1a,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1Priority,1,01,00,00,00
 
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,NumOfPorts,1,01,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1,1,24,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1,1,23,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1Priority,1,02,00,00,00
 
[Oem.NICO3.AddReg]
HKR,Settings\OEM,Flags,1,72,38,00,5A
HKR,Settings\OEM,Flags2,1,A0,31,B4,63
HKR,Settings\OEM,Flags3,1,80,08,02,10
HKR,Settings\OEM,Flags4,1,80,78,10,00
HKR,Settings\OEM,Flags5,1,00,04,41,00
HKR,Settings\OEM,PortsCap,1,00,27,27,00
HKR,Settings\OEM,EqProfile,1,01,00,00,00
HKR,Settings\OEM,SmartAudioSettings,1,D0,11,00,00
HKR,Settings\OEM,NumOfSoftStream,1,01,01,00,00
HKR,Settings\OEM,DefaultGain,1,13,00,2B,14,00,00,00,00
HKR,Settings\OEM,DefaultAECMicLowLevel,1,00,00,00,00
HKR,Settings\OEM,DefaultAECMicHighLevel,1,00,00,18,00
HKR,Settings\OEM,SASpatializerPhantomSPSpread,1,40,00,00,00
HKR,Settings\OEM,SASpatializerImmersionSpread,1,40,00,00,00
HKR,Settings\OEM,TestRegBypassIndex,1,1A,00,00,00,00,00,00,00
HKR,Settings\OEM\DefaultJack,Wid19,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1A,1,0a,00,00,02 
HKR,Settings\OEM\DefaultJack,Wid1B,1,0a,00,00,01 
HKR,Settings\OEM\DefaultJack,Wid1C,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1D,1,01,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1E,1,0a,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1F,1,01,00,01,00
HKR,Settings\OEM\DefaultJack,Wid23,1,0a,00,01,00 
HKR,Settings\OEM\DefaultJack,Wid27,1,0a,00,00,00 
HKR,Settings\OEM\InitialSliderPosition,InitialMasterPlaybackPos,1,C9,7A,F8,FF
HKR,Settings\OEM\InitialSliderPosition,InitialLineInPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialWaveOutMixCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxCapturePos,1,C9,FA,0E,00
HKR,Settings\OEM\InitialSliderPosition,InitialLineInCapturePos,1,C9,7A,10,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicCapturePos,1,00,00,06,00
HKR,Settings\OEM\InitialSliderPosition,InitialCDCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicBoostCapturePos,1,00,00,24,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxMicBoostCapturePos,1,00,00,1E,00
 
;default Min for Pebble is 0xffb60000(-74dB), default Max for Pebble is 0x60000(+6dB)
;default Min for Venice is 0x00000000(0dB), default Max for Venice is 0x228000(+34.5dB)
;default Min for Waikiki is 0x00000000(0dB), default Max for Waikiki is 0x150000(+21dB)
;note 0x10000=1dB, 0x8000=0.5dB
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMax,1,00,00,06,00 
HKR,Settings\OEM\MicInRange,DigiMicBoostOffset,1,00,00,EC,FF
HKR,Settings\OEM\MicInRange,IntMicDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortBDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortCDefaultBoostGainStep,1,02,00,00,00
 
HKR,Settings\OEM\MicInRange,PortAMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortAMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortBMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBBoostOffset,1,00,00,02,00
HKR,Settings\OEM\MicInRange,PortCMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortCMicInMax,1,00,00,16,00	
HKR,Settings\OEM\MicInRange,PortCBoostOffset,1,00,00,F8,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMax,1,00,00,06,00	
 
HKR,Settings\OEM\LineInRange,PortALineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortALineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortBLineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortBLineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortCLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortCLineInMax,1,00,00,06,00	
HKR,Settings\OEM\LineInRange,PortFLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortFLineInMax,1,00,00,06,00	
 
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMin,1,00,00,00,00
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMax,1,00,80,22,00
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMin,1,00,00,A0,FF
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMax,1,00,00,0C,00
 
;    64 = 100% of the volume possible,etc...
;    32 = 50% of the volume possible,etc...
HKR,Settings\OEM\FlexSettings,Flex_MasterPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDPlaybackVolume,0x00000001,2D,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_WaveOutMixCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_AuxCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDCaptureVolume,0x00000001,64,00,00,00
 
; PortRules changed to ULONGLONG, 64bits
HKR,Settings\PortRules,NumOfRules,1,07,00,00,00
HKR,Settings\PortRules,PortRules,1,\
11,62,6F,6F,62,6F,6F,51,\
10,52,6F,6F,72,6F,6F,71,\
10,52,6F,6F,62,6F,6F,71,\
10,62,6F,6F,52,6F,6F,71,\
90,52,4F,4F,52,4F,4F,71,\
90,52,4F,4F,42,4F,4F,51,\
90,42,4F,4F,52,4F,4F,51
 
HKR,Settings\MicInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\MicInPortRules,PortRules,1,\
10,4F,3A,4F,4F,4F,0A,4F,\
10,4F,0A,4F,4F,4F,3A,4F
 
HKR,Settings\LineInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\LineInPortRules,PortRules,1,\
10,4F,4F,08,4F,4F,4F,4F,\
10,4F,4F,58,4F,4F,4F,4F
 
;PEBBLE port configuration settings
HKR,Settings\PortConfig\ClassicModeCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,NumOfPorts,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1,1,1e,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2,1,23,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3,1,1a,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4,1,1b,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1Priority,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2Priority,1,03,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3Priority,1,02,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1,1,1b,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection2,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1,1,1a,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1Priority,1,01,00,00,00
 
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,NumOfPorts,1,01,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1,1,24,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1,1,23,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1Priority,1,02,00,00,00
 
[Oem.MOCA3.AddReg]
HKR,Settings\OEM,Flags,1,72,38,00,5A
HKR,Settings\OEM,Flags2,1,A2,31,B4,63
HKR,Settings\OEM,Flags3,1,80,08,02,10
HKR,Settings\OEM,Flags4,1,80,78,10,00
HKR,Settings\OEM,Flags5,1,00,06,41,00
HKR,Settings\OEM,PortsCap,1,00,27,27,00
HKR,Settings\OEM,EqProfile,1,01,00,00,00
HKR,Settings\OEM,SmartAudioSettings,1,D0,11,00,00
HKR,Settings\OEM,NumOfSoftStream,1,01,01,00,00
HKR,Settings\OEM,DefaultGain,1,13,00,2B,14,00,00,00,00
HKR,Settings\OEM,DefaultAECMicLowLevel,1,00,00,00,00
HKR,Settings\OEM,DefaultAECMicHighLevel,1,00,00,18,00
HKR,Settings\OEM,SASpatializerPhantomSPSpread,1,40,00,00,00
HKR,Settings\OEM,SASpatializerImmersionSpread,1,40,00,00,00
HKR,Settings\OEM,TestRegBypassIndex,1,1A,00,00,00,00,00,00,00
HKR,Settings\OEM\DefaultJack,Wid19,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1A,1,0a,00,00,02 
HKR,Settings\OEM\DefaultJack,Wid1B,1,0a,00,00,01 
HKR,Settings\OEM\DefaultJack,Wid1C,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1D,1,01,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1E,1,0a,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1F,1,01,00,01,00
HKR,Settings\OEM\DefaultJack,Wid23,1,0a,00,01,00 
HKR,Settings\OEM\DefaultJack,Wid27,1,0a,00,00,00 
HKR,Settings\OEM\InitialSliderPosition,InitialMasterPlaybackPos,1,C9,7A,F8,FF
HKR,Settings\OEM\InitialSliderPosition,InitialLineInPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialWaveOutMixCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxCapturePos,1,C9,FA,0E,00
HKR,Settings\OEM\InitialSliderPosition,InitialLineInCapturePos,1,C9,7A,10,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicCapturePos,1,00,00,06,00
HKR,Settings\OEM\InitialSliderPosition,InitialCDCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicBoostCapturePos,1,00,00,24,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxMicBoostCapturePos,1,00,00,1E,00
 
;default Min for Pebble is 0xffb60000(-74dB), default Max for Pebble is 0x60000(+6dB)
;default Min for Venice is 0x00000000(0dB), default Max for Venice is 0x228000(+34.5dB)
;default Min for Waikiki is 0x00000000(0dB), default Max for Waikiki is 0x150000(+21dB)
;note 0x10000=1dB, 0x8000=0.5dB
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMax,1,00,00,06,00 
HKR,Settings\OEM\MicInRange,DigiMicBoostOffset,1,00,00,EC,FF
HKR,Settings\OEM\MicInRange,IntMicDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortBDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortCDefaultBoostGainStep,1,02,00,00,00
 
HKR,Settings\OEM\MicInRange,PortAMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortAMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortBMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBBoostOffset,1,00,00,02,00
HKR,Settings\OEM\MicInRange,PortCMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortCMicInMax,1,00,00,16,00
HKR,Settings\OEM\MicInRange,PortCBoostOffset,1,00,00,F8,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMax,1,00,00,06,00	
 
HKR,Settings\OEM\LineInRange,PortALineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortALineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortBLineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortBLineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortCLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortCLineInMax,1,00,00,06,00	
HKR,Settings\OEM\LineInRange,PortFLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortFLineInMax,1,00,00,06,00	
 
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMin,1,00,00,00,00
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMax,1,00,80,22,00
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMin,1,00,00,A0,FF
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMax,1,00,00,0C,00
 
;    64 = 100% of the volume possible,etc...
;    32 = 50% of the volume possible,etc...
HKR,Settings\OEM\FlexSettings,Flex_MasterPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDPlaybackVolume,0x00000001,2D,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_WaveOutMixCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_AuxCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDCaptureVolume,0x00000001,64,00,00,00
 
; PortRules changed to ULONGLONG, 64bits
HKR,Settings\PortRules,NumOfRules,1,0C,00,00,00
HKR,Settings\PortRules,PortRules,1,\
11,62,6F,6F,62,61,6F,51,\
10,52,6F,6F,62,61,6F,71,\
10,62,6F,6F,62,51,6F,71,\
10,52,6F,6F,62,71,6F,71,\
10,62,6F,6F,52,61,6F,71,\
10,62,6F,6F,52,71,6F,71,\
10,52,6F,6F,72,61,6F,71,\
10,52,6F,6F,72,71,6F,71,\
90,52,4F,4F,72,51,4F,71,\
90,62,4F,4F,52,51,4F,51,\
90,52,4F,4F,52,61,4F,71,\
90,52,4F,4F,52,71,4F,71
 
HKR,Settings\MicInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\MicInPortRules,PortRules,1,\
10,4F,3A,4F,4F,4F,0A,4F,\
10,4F,0A,4F,4F,4F,3A,4F
 
HKR,Settings\LineInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\LineInPortRules,PortRules,1,\
10,4F,4F,08,4F,4F,4F,4F,\
10,4F,4F,58,4F,4F,4F,4F
 
;PEBBLE port configuration settings
HKR,Settings\PortConfig\ClassicModeCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,NumOfPorts,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1,1,1e,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2,1,23,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3,1,1a,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4,1,1b,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1Priority,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2Priority,1,03,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3Priority,1,02,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1,1,1b,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection2,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1,1,1a,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1Priority,1,01,00,00,00
 
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,NumOfPorts,1,01,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1,1,24,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1,1,23,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1Priority,1,02,00,00,00
 
[Oem.PCAN3.AddReg]
HKR,Settings\OEM,Flags,1,72,38,00,5A
HKR,Settings\OEM,Flags2,1,A2,31,B4,63
HKR,Settings\OEM,Flags3,1,80,08,02,10
HKR,Settings\OEM,Flags4,1,80,78,10,00
HKR,Settings\OEM,Flags5,1,00,06,41,00
HKR,Settings\OEM,PortsCap,1,00,27,27,00
HKR,Settings\OEM,EqProfile,1,01,00,00,00
HKR,Settings\OEM,SmartAudioSettings,1,D0,11,00,00
HKR,Settings\OEM,NumOfSoftStream,1,01,01,00,00
HKR,Settings\OEM,DefaultGain,1,13,00,2B,14,00,00,00,00
HKR,Settings\OEM,DefaultAECMicLowLevel,1,00,00,00,00
HKR,Settings\OEM,DefaultAECMicHighLevel,1,00,00,18,00
HKR,Settings\OEM,SASpatializerPhantomSPSpread,1,40,00,00,00
HKR,Settings\OEM,SASpatializerImmersionSpread,1,40,00,00,00
HKR,Settings\OEM,TestRegBypassIndex,1,1A,00,00,00,00,00,00,00
HKR,Settings\OEM\DefaultJack,Wid19,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1A,1,0a,00,00,02 
HKR,Settings\OEM\DefaultJack,Wid1B,1,0a,00,00,01 
HKR,Settings\OEM\DefaultJack,Wid1C,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1D,1,01,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1E,1,0a,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1F,1,01,00,01,00
HKR,Settings\OEM\DefaultJack,Wid23,1,0a,00,01,00 
HKR,Settings\OEM\DefaultJack,Wid27,1,0a,00,00,00 
HKR,Settings\OEM\InitialSliderPosition,InitialMasterPlaybackPos,1,C9,7A,F8,FF
HKR,Settings\OEM\InitialSliderPosition,InitialLineInPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialWaveOutMixCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxCapturePos,1,C9,FA,0E,00
HKR,Settings\OEM\InitialSliderPosition,InitialLineInCapturePos,1,C9,7A,10,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicCapturePos,1,00,00,06,00
HKR,Settings\OEM\InitialSliderPosition,InitialCDCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicBoostCapturePos,1,00,00,24,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxMicBoostCapturePos,1,00,00,1E,00
 
;default Min for Pebble is 0xffb60000(-74dB), default Max for Pebble is 0x60000(+6dB)
;default Min for Venice is 0x00000000(0dB), default Max for Venice is 0x228000(+34.5dB)
;default Min for Waikiki is 0x00000000(0dB), default Max for Waikiki is 0x150000(+21dB)
;note 0x10000=1dB, 0x8000=0.5dB
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMax,1,00,00,06,00 
HKR,Settings\OEM\MicInRange,DigiMicBoostOffset,1,00,00,F0,FF
HKR,Settings\OEM\MicInRange,IntMicDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortBDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortCDefaultBoostGainStep,1,02,00,00,00
 
HKR,Settings\OEM\MicInRange,PortAMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortAMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortBMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBBoostOffset,1,00,00,02,00
HKR,Settings\OEM\MicInRange,PortCMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortCMicInMax,1,00,00,16,00
HKR,Settings\OEM\MicInRange,PortCBoostOffset,1,00,00,F8,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMax,1,00,00,06,00	
 
HKR,Settings\OEM\LineInRange,PortALineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortALineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortBLineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortBLineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortCLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortCLineInMax,1,00,00,06,00	
HKR,Settings\OEM\LineInRange,PortFLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortFLineInMax,1,00,00,06,00	
 
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMin,1,00,00,00,00
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMax,1,00,80,22,00
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMin,1,00,00,A0,FF
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMax,1,00,00,0C,00
 
;    64 = 100% of the volume possible,etc...
;    32 = 50% of the volume possible,etc...
HKR,Settings\OEM\FlexSettings,Flex_MasterPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDPlaybackVolume,0x00000001,2D,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_WaveOutMixCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_AuxCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDCaptureVolume,0x00000001,64,00,00,00
 
; PortRules changed to ULONGLONG, 64bits
HKR,Settings\PortRules,NumOfRules,1,0C,00,00,00
HKR,Settings\PortRules,PortRules,1,\
11,62,6F,6F,62,61,6F,51,\
10,52,6F,6F,62,61,6F,71,\
10,62,6F,6F,62,51,6F,71,\
10,52,6F,6F,62,71,6F,71,\
10,62,6F,6F,52,61,6F,71,\
10,62,6F,6F,52,71,6F,71,\
10,52,6F,6F,72,61,6F,71,\
10,52,6F,6F,72,71,6F,71,\
90,52,4F,4F,72,51,4F,71,\
90,62,4F,4F,52,51,4F,51,\
90,52,4F,4F,52,61,4F,71,\
90,52,4F,4F,52,71,4F,71
 
HKR,Settings\MicInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\MicInPortRules,PortRules,1,\
10,4F,3A,4F,4F,4F,0A,4F,\
10,4F,0A,4F,4F,4F,3A,4F
 
HKR,Settings\LineInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\LineInPortRules,PortRules,1,\
10,4F,4F,08,4F,4F,4F,4F,\
10,4F,4F,58,4F,4F,4F,4F
 
;PEBBLE port configuration settings
HKR,Settings\PortConfig\ClassicModeCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,NumOfPorts,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1,1,1e,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2,1,23,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3,1,1a,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4,1,1b,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1Priority,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2Priority,1,03,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3Priority,1,02,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1,1,1b,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection2,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1,1,1a,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1Priority,1,01,00,00,00
 
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,NumOfPorts,1,01,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1,1,24,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1,1,23,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1Priority,1,02,00,00,00
 
[Oem.CRML3.AddReg]
HKR,Settings\OEM,Flags,1,72,38,00,5A
HKR,Settings\OEM,Flags2,1,A2,31,B4,7F
HKR,Settings\OEM,Flags3,1,80,08,02,10
HKR,Settings\OEM,Flags4,1,80,78,10,00
HKR,Settings\OEM,Flags5,1,00,06,41,00
HKR,Settings\OEM,PortsCap,1,00,27,27,00
HKR,Settings\OEM,EqProfile,1,01,00,00,00
HKR,Settings\OEM,SmartAudioSettings,1,D8,11,00,00
HKR,Settings\OEM,NumOfSoftStream,1,01,01,00,00
HKR,Settings\OEM,DefaultGain,1,13,00,2B,14,00,00,00,00
HKR,Settings\OEM,DefaultAECMicLowLevel,1,00,00,00,00
HKR,Settings\OEM,DefaultAECMicHighLevel,1,00,00,18,00
HKR,Settings\OEM,SASpatializerPhantomSPSpread,1,40,00,00,00
HKR,Settings\OEM,SASpatializerImmersionSpread,1,40,00,00,00
HKR,Settings\OEM,TestRegBypassIndex,1,1A,00,00,00,00,00,00,00
HKR,Settings\OEM\DefaultJack,Wid19,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1A,1,0a,00,00,02 
HKR,Settings\OEM\DefaultJack,Wid1B,1,0a,00,00,01 
HKR,Settings\OEM\DefaultJack,Wid1C,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1D,1,01,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1E,1,0a,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1F,1,01,00,01,00
HKR,Settings\OEM\DefaultJack,Wid23,1,0a,00,01,00 
HKR,Settings\OEM\DefaultJack,Wid27,1,0a,00,00,00 
HKR,Settings\OEM\InitialSliderPosition,InitialMasterPlaybackPos,1,C9,7A,F8,FF
HKR,Settings\OEM\InitialSliderPosition,InitialLineInPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialWaveOutMixCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxCapturePos,1,C9,FA,0E,00
HKR,Settings\OEM\InitialSliderPosition,InitialLineInCapturePos,1,C9,7A,10,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicCapturePos,1,00,00,06,00
HKR,Settings\OEM\InitialSliderPosition,InitialCDCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicBoostCapturePos,1,00,00,24,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxMicBoostCapturePos,1,00,00,1E,00
 
;default Min for Pebble is 0xffb60000(-74dB), default Max for Pebble is 0x60000(+6dB)
;default Min for Venice is 0x00000000(0dB), default Max for Venice is 0x228000(+34.5dB)
;default Min for Waikiki is 0x00000000(0dB), default Max for Waikiki is 0x150000(+21dB)
;note 0x10000=1dB, 0x8000=0.5dB
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,DigiMicBoostOffset,1,00,00,EC,FF 
HKR,Settings\OEM\MicInRange,IntMicDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortBDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortCDefaultBoostGainStep,1,02,00,00,00
 
HKR,Settings\OEM\MicInRange,PortAMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortAMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortBMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBBoostOffset,1,00,00,02,00
HKR,Settings\OEM\MicInRange,PortCMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortCMicInMax,1,00,00,16,00
HKR,Settings\OEM\MicInRange,PortCBoostOffset,1,00,00,F8,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMax,1,00,00,06,00	
 
HKR,Settings\OEM\LineInRange,PortALineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortALineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortBLineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortBLineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortCLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortCLineInMax,1,00,00,06,00	
HKR,Settings\OEM\LineInRange,PortFLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortFLineInMax,1,00,00,06,00	
 
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMin,1,00,00,00,00
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMax,1,00,80,22,00
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMin,1,00,00,A0,FF
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMax,1,00,00,0C,00
 
;    64 = 100% of the volume possible,etc...
;    32 = 50% of the volume possible,etc...
HKR,Settings\OEM\FlexSettings,Flex_MasterPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDPlaybackVolume,0x00000001,2D,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_WaveOutMixCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_AuxCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDCaptureVolume,0x00000001,64,00,00,00
 
; PortRules changed to ULONGLONG, 64bits
HKR,Settings\PortRules,NumOfRules,1,0C,00,00,00
HKR,Settings\PortRules,PortRules,1,\
11,62,6F,6F,62,61,6F,51,\
10,52,6F,6F,62,61,6F,71,\
10,62,6F,6F,62,51,6F,71,\
10,52,6F,6F,62,71,6F,71,\
10,62,6F,6F,52,61,6F,71,\
10,62,6F,6F,52,71,6F,71,\
10,52,6F,6F,72,61,6F,71,\
10,52,6F,6F,72,71,6F,71,\
90,52,4F,4F,72,51,4F,71,\
90,62,4F,4F,52,51,4F,51,\
90,52,4F,4F,52,61,4F,71,\
90,52,4F,4F,52,71,4F,71
 
HKR,Settings\MicInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\MicInPortRules,PortRules,1,\
10,4F,3A,4F,4F,4F,0A,4F,\
10,4F,0A,4F,4F,4F,3A,4F
 
HKR,Settings\LineInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\LineInPortRules,PortRules,1,\
10,4F,4F,08,4F,4F,4F,4F,\
10,4F,4F,58,4F,4F,4F,4F
 
;PEBBLE port configuration settings
HKR,Settings\PortConfig\ClassicModeCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,NumOfPorts,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1,1,1e,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2,1,23,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3,1,1a,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4,1,1b,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1Priority,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2Priority,1,03,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3Priority,1,02,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1,1,1b,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection2,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1,1,1a,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1Priority,1,01,00,00,00
 
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,NumOfPorts,1,01,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1,1,24,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1,1,23,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1Priority,1,02,00,00,00
 
[Oem.KNDO.AddReg]
HKR,Settings\OEM,Flags,1,72,38,00,5A
HKR,Settings\OEM,Flags2,1,A2,31,B4,7F
HKR,Settings\OEM,Flags3,1,80,08,02,10
HKR,Settings\OEM,Flags4,1,80,78,10,00
HKR,Settings\OEM,Flags5,1,00,04,41,00
HKR,Settings\OEM,PortsCap,1,00,27,27,00
HKR,Settings\OEM,EqProfile,1,01,00,00,00
HKR,Settings\OEM,SmartAudioSettings,1,D8,11,00,00
HKR,Settings\OEM,NumOfSoftStream,1,01,01,00,00
HKR,Settings\OEM,DefaultGain,1,13,00,2B,14,00,00,00,00
HKR,Settings\OEM,DefaultAECMicLowLevel,1,00,00,00,00
HKR,Settings\OEM,DefaultAECMicHighLevel,1,00,00,18,00
HKR,Settings\OEM,SASpatializerPhantomSPSpread,1,40,00,00,00
HKR,Settings\OEM,SASpatializerImmersionSpread,1,40,00,00,00
HKR,Settings\OEM,TestRegBypassIndex,1,1A,00,00,00,00,00,00,00
HKR,Settings\OEM\DefaultJack,Wid19,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1A,1,0a,00,00,02 
HKR,Settings\OEM\DefaultJack,Wid1B,1,0a,00,00,01 
HKR,Settings\OEM\DefaultJack,Wid1C,1,02,00,00,00
HKR,Settings\OEM\DefaultJack,Wid1D,1,01,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1E,1,0a,00,00,00 
HKR,Settings\OEM\DefaultJack,Wid1F,1,01,00,01,00
HKR,Settings\OEM\DefaultJack,Wid23,1,0a,00,01,00 
HKR,Settings\OEM\DefaultJack,Wid27,1,0a,00,00,00 
HKR,Settings\OEM\InitialSliderPosition,InitialMasterPlaybackPos,1,C9,7A,F8,FF
HKR,Settings\OEM\InitialSliderPosition,InitialLineInPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicPlaybackPos,1,C9,7A,04,00
HKR,Settings\OEM\InitialSliderPosition,InitialWaveOutMixCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxCapturePos,1,C9,FA,0E,00
HKR,Settings\OEM\InitialSliderPosition,InitialLineInCapturePos,1,C9,7A,10,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicCapturePos,1,00,00,06,00
HKR,Settings\OEM\InitialSliderPosition,InitialCDCapturePos,1,C9,7A,1C,00
HKR,Settings\OEM\InitialSliderPosition,InitialMicBoostCapturePos,1,00,00,24,00
HKR,Settings\OEM\InitialSliderPosition,InitialAuxMicBoostCapturePos,1,00,00,1E,00
 
;default Min for Pebble is 0xffb60000(-74dB), default Max for Pebble is 0x60000(+6dB)
;default Min for Venice is 0x00000000(0dB), default Max for Venice is 0x228000(+34.5dB)
;default Min for Waikiki is 0x00000000(0dB), default Max for Waikiki is 0x150000(+21dB)
;note 0x10000=1dB, 0x8000=0.5dB
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedExternalMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,DedicatedInternalMicInMax,1,00,00,06,00 
HKR,Settings\OEM\MicInRange,DigiMicBoostOffset,1,00,00,EC,FF
HKR,Settings\OEM\MicInRange,IntMicDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortBDefaultBoostGainStep,1,02,00,00,00
HKR,Settings\OEM\MicInRange,PortCDefaultBoostGainStep,1,02,00,00,00
 
HKR,Settings\OEM\MicInRange,PortAMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortAMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBMicInMin,1,00,00,B6,FF
HKR,Settings\OEM\MicInRange,PortBMicInMax,1,00,00,06,00
HKR,Settings\OEM\MicInRange,PortBBoostOffset,1,00,00,02,00
HKR,Settings\OEM\MicInRange,PortCMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortCMicInMax,1,00,00,16,00
HKR,Settings\OEM\MicInRange,PortCBoostOffset,1,00,00,F8,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMin,1,00,00,B6,FF	
HKR,Settings\OEM\MicInRange,PortFMicInMax,1,00,00,06,00	

HKR,Settings\OEM\LineInRange,PortALineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortALineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortBLineInMin,1,00,00,B6,FF
HKR,Settings\OEM\LineInRange,PortBLineInMax,1,00,00,06,00
HKR,Settings\OEM\LineInRange,PortCLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortCLineInMax,1,00,00,06,00	
HKR,Settings\OEM\LineInRange,PortFLineInMin,1,00,00,B6,FF	
HKR,Settings\OEM\LineInRange,PortFLineInMax,1,00,00,06,00	

HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMin,1,00,00,00,00
HKR,Settings\OEM\CDWaveInRange,DedicatedCDInMax,1,00,80,22,00
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMin,1,00,00,A0,FF
HKR,Settings\OEM\CDWaveInRange,DedicatedWaveInMax,1,00,00,0C,00

;    64 = 100% of the volume possible,etc...
;    32 = 50% of the volume possible,etc...
HKR,Settings\OEM\FlexSettings,Flex_MasterPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicPlaybackVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDPlaybackVolume,0x00000001,2D,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_WaveOutMixCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_AuxCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_LineInCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_MicCaptureVolume,0x00000001,64,00,00,00
HKR,Settings\OEM\FlexSettings,Flex_CDCaptureVolume,0x00000001,64,00,00,00

; PortRules changed to ULONGLONG, 64bits
HKR,Settings\PortRules,NumOfRules,1,07,00,00,00
HKR,Settings\PortRules,PortRules,1,\
11,62,6F,6F,62,6F,6F,51,\
10,52,6F,6F,72,6F,6F,71,\
10,52,6F,6F,62,6F,6F,71,\
10,62,6F,6F,52,6F,6F,71,\
90,52,4F,4F,52,4F,4F,71,\
90,52,4F,4F,42,4F,4F,51,\
90,42,4F,4F,52,4F,4F,51
 
HKR,Settings\MicInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\MicInPortRules,PortRules,1,\
10,4F,3A,4F,4F,4F,0A,4F,\
10,4F,0A,4F,4F,4F,3A,4F

HKR,Settings\LineInPortRules,NumOfRules,1,02,00,00,00
HKR,Settings\LineInPortRules,PortRules,1,\
10,4F,4F,08,4F,4F,4F,4F,\
10,4F,4F,58,4F,4F,4F,4F

;PEBBLE port configuration settings
HKR,Settings\PortConfig\ClassicModeCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,NumOfPorts,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1,1,1e,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2,1,23,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3,1,1a,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4,1,1b,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port1Priority,1,04,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port2Priority,1,03,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port3Priority,1,02,00,00,00
HKR,Settings\PortConfig\ClassicModeCollection1\MicSubDevice,Port4Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1,1,1b,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection1\MicSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\AnalogDigitalCollection2,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1,1,1a,00,00,00
HKR,Settings\PortConfig\AnalogDigitalCollection2\MicSubDevice,Port1Priority,1,01,00,00,00
 
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,NumOfPorts,1,01,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1,1,24,00,00,00
;HKR,Settings\PortConfig\AnalogDigitalCollection2\SumSubDevice,Port1Priority,1,01,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1,NumOfSubDevices,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialSliderPos,1,00,00,10,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,InitialBoostSliderPos,1,00,00,1E,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,NumOfPorts,1,01,00,00,00
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1,1,23,00,00,00
 
HKR,Settings\PortConfig\DigitalCollection1\MicSubDevice,Port1Priority,1,02,00,00,00
 
[AECDRC.AddReg]
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\AECDRC,Threshold,0x00010001,00,00,00,c0
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\AECDRC,MaxInputLevel,0x00010001,00,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\AECDRC,MaxOutputLevel,0x00010001,00,00,40,c0
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\AECDRC,AttackTime,0x00010001,14,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\AECDRC,ReleaseTime,0x00010001,00,14,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\AECDRC,LinearGain,0x00010001,00,00,00,00

[LnVoIP.AddReg]
HKLM, Software\Lenovo\Audio\Integrated,CplDirectory,, "%16422%\Conexant\SAII"
HKLM, Software\Lenovo\Audio\Integrated,CplExeFile,, "%16422%\Conexant\SAII\SAIICpl.exe"
HKLM, Software\Lenovo\Audio\Integrated,CplParam,, ""
HKLM, Software\Lenovo\Audio\Integrated,CplKeyFile,, "%16422%\Conexant\SAII\SmartAudio.exe"

[SoftEQ.SHINMV.AddReg]
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1,SystemName,,ShinaiMV
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ProfileName,,default int spk
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,SpeakerApplication,,InternalSpeaker

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Cancel,0x00010001,00,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Channel,0x00010001,09,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,NumBands,0x00010001,0a,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolRight,0x00010001,ff,7f,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolLeft,0x00010001,ff,7f,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,LinearGain,0x00010001,00,00,90,40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,DRCEnable,0x00010001,01,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Threshold,0x00010001,00,00,20,c0
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxInputLevel,0x00010001,00,00,40,40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxOutputLevel,0x00010001,c1,cc,cc,bd
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTime,0x00010001,50,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTime,0x00010001,00,14,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags1,0x00010001,04,01,01,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq1,0x00010001,d2,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1001,0x00010001,64,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1001,0x00010001,00,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags1,0x00010001,00,01,02,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq1,0x00010001,3e,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1001,0x00010001,64,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1001,0x00010001,00,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags1,0x00010001,00,01,04,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq1,0x00010001,ee,02,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1001,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1001,0x00010001,40,01,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags1,0x00010001,00,01,08,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq1,0x00010001,fa,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1001,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1001,0x00010001,5e,01,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags1,0x00010001,00,01,10,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq1,0x00010001,5e,01,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1001,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1001,0x00010001,cb,01,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags1,0x00010001,00,01,20,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq1,0x00010001,e8,03,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1001,0x00010001,64,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1001,0x00010001,25,ff,ff,ff

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags1,0x00010001,00,01,40,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq1,0x00010001,c4,09,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1001,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1001,0x00010001,96,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags1,0x00010001,00,01,80,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq1,0x00010001,e4,0c,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1001,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1001,0x00010001,96,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags1,0x00010001,00,01,00,01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq1,0x00010001,a0,0f,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1001,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1001,0x00010001,96,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags1,0x00010001,00,01,00,02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq1,0x00010001,40,1f,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1001,0x00010001,64,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1001,0x00010001,6b,ff,ff,ff

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags2,0x00010001,04,02,01,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq2,0x00010001,d2,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1002,0x00010001,64,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1002,0x00010001,00,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags2,0x00010001,00,02,02,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq2,0x00010001,3e,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1002,0x00010001,64,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1002,0x00010001,00,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags2,0x00010001,00,02,04,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq2,0x00010001,ee,02,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1002,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1002,0x00010001,40,01,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags2,0x00010001,00,02,08,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq2,0x00010001,fa,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1002,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1002,0x00010001,5e,01,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags2,0x00010001,00,02,10,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq2,0x00010001,5e,01,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1002,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1002,0x00010001,cb,01,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags2,0x00010001,00,02,20,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq2,0x00010001,e8,03,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1002,0x00010001,64,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1002,0x00010001,25,ff,ff,ff

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags2,0x00010001,00,02,40,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq2,0x00010001,c4,09,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1002,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1002,0x00010001,96,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags2,0x00010001,00,02,80,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq2,0x00010001,e4,0c,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1002,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1002,0x00010001,96,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags2,0x00010001,00,02,00,01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq2,0x00010001,a0,0f,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1002,0x00010001,4b,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1002,0x00010001,96,00,00,00

HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags2,0x00010001,00,02,00,02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq2,0x00010001,40,1f,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1002,0x00010001,64,00,00,00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1002,0x00010001,6b,ff,ff,ff

[SoftEQ.NZMI1.AddReg]
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1,SystemName,,NZMI1
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ProfileName,,default int spk
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,SpeakerApplication,,InternalSpeaker
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Cancel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Channel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,NumBands,0x00010001, 0A, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolLeft,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolRight,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,DRCEnable,0x00010001, 01, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTime,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTimeInMS,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTime,0x00010001, 00, 14, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTimeInMS,0x00010001, 00, 14, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Threshold,0x00010001, 00, 00, 80, BF
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,LinearGain,0x00010001, 00, 00, A0, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxInputLevel,0x00010001, 00, 00, B0, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxOutputLevel,0x00010001, 00, 98, 99, BE
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags1,0x00010001, 04, 01, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq1,0x00010001, C8, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags1,0x00010001, 00, 01, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq1,0x00010001, 3E, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags1,0x00010001, 00, 01, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq1,0x00010001, B2, 02, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1001,0x00010001, 6E, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1001,0x00010001, 08, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags1,0x00010001, 00, 01, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq1,0x00010001, 45, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1001,0x00010001, DC, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags1,0x00010001, 00, 01, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq1,0x00010001, C4, 09, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1001,0x00010001, A0, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags1,0x00010001, 00, 01, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq1,0x00010001, E8, 03, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1001,0x00010001, DC, FD, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags1,0x00010001, 00, 01, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq1,0x00010001, D0, 07, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1001,0x00010001, 5E, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags1,0x00010001, 00, 01, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq1,0x00010001, DC, 05, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1001,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1001,0x00010001, A3, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags1,0x00010001, 00, 01, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq1,0x00010001, 40, 1F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1001,0x00010001, 28, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags1,0x00010001, 02, 01, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq1,0x00010001, 10, 27, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1001,0x00010001, 26, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags2,0x00010001, 04, 02, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq2,0x00010001, C8, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags2,0x00010001, 00, 02, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq2,0x00010001, 3E, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags2,0x00010001, 00, 02, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq2,0x00010001, B2, 02, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1002,0x00010001, 6E, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1002,0x00010001, 08, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags2,0x00010001, 00, 02, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq2,0x00010001, 45, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1002,0x00010001, DC, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags2,0x00010001, 00, 02, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq2,0x00010001, C4, 09, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1002,0x00010001, A0, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags2,0x00010001, 00, 02, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq2,0x00010001, E8, 03, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1002,0x00010001, DC, FD, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags2,0x00010001, 00, 02, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq2,0x00010001, D0, 07, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1002,0x00010001, 5E, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags2,0x00010001, 00, 02, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq2,0x00010001, DC, 05, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1002,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1002,0x00010001, A3, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags2,0x00010001, 00, 02, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq2,0x00010001, 40, 1F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1002,0x00010001, 28, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags2,0x00010001, 02, 02, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq2,0x00010001, 10, 27, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1002,0x00010001, 26, 02, 00, 00
 
[SoftEQ.NICO3.AddReg]
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1,SystemName,,NICO3
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ProfileName,,default int spk
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,SpeakerApplication,,InternalSpeaker
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Cancel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Channel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,NumBands,0x00010001, 0A, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolLeft,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolRight,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,DRCEnable,0x00010001, 01, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTime,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTimeInMS,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTime,0x00010001, 00, 14, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTimeInMS,0x00010001, 00, 14, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Threshold,0x00010001, 00, 00, 80, BF
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Boost,0x00010001, 00, 00, 40, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxInputLevel,0x00010001, 00, 00, F0, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxOutputLevel,0x00010001, 00, 98, 99, BE
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags1,0x00010001, 04, 01, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq1,0x00010001, A0, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags1,0x00010001, 04, 01, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq1,0x00010001, A0, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags1,0x00010001, 00, 01, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq1,0x00010001, 6C, 02, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1001,0x00010001, 6E, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1001,0x00010001, 95, FD, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags1,0x00010001, 00, 01, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq1,0x00010001, 45, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1001,0x00010001, 26, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags1,0x00010001, 00, 01, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq1,0x00010001, 0C, 03, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1001,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1001,0x00010001, 9D, FF, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags1,0x00010001, 00, 01, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq1,0x00010001, 28, 05, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1001,0x00010001, 26, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags1,0x00010001, 00, 01, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq1,0x00010001, D0, 07, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1001,0x00010001, DC, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags1,0x00010001, 00, 01, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq1,0x00010001, A0, 0F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1001,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags1,0x00010001, 00, 01, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq1,0x00010001, 7C, 15, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1001,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1001,0x00010001, 5E, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags1,0x00010001, 00, 01, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq1,0x00010001, 10, 27, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1001,0x00010001, 1F, FF, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags2,0x00010001, 04, 02, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq2,0x00010001, A0, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags2,0x00010001, 04, 02, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq2,0x00010001, A0, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags2,0x00010001, 00, 02, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq2,0x00010001, 6C, 02, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1002,0x00010001, 6E, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1002,0x00010001, 95, FD, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags2,0x00010001, 00, 02, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq2,0x00010001, 45, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1002,0x00010001, 26, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags2,0x00010001, 00, 02, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq2,0x00010001, 0C, 03, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1002,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1002,0x00010001, 9D, FF, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags2,0x00010001, 00, 02, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq2,0x00010001, 28, 05, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1002,0x00010001, 26, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags2,0x00010001, 00, 02, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq2,0x00010001, D0, 07, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1002,0x00010001, DC, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags2,0x00010001, 00, 02, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq2,0x00010001, A0, 0F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1002,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags2,0x00010001, 00, 02, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq2,0x00010001, 7C, 15, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1002,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1002,0x00010001, 5E, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags2,0x00010001, 00, 02, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq2,0x00010001, 10, 27, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1002,0x00010001, 1F, FF, FF, FF
 
[SoftEQ.MOCA3.AddReg]
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1,SystemName,,MOCA3
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ProfileName,,default int spk
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,SpeakerApplication,,InternalSpeaker
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Cancel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Channel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,NumBands,0x00010001, 0A, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolLeft,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolRight,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,DRCEnable,0x00010001, 01, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTime,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTimeInMS,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTime,0x00010001, 00, 14, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTimeInMS,0x00010001, 00, 14, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Threshold,0x00010001, 00, 00, 80, BF
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,LinearGain,0x00010001, 00, 00, 20, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxInputLevel,0x00010001, 00, 00, D8, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxOutputLevel,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags1,0x00010001, 04, 01, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq1,0x00010001, AA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags1,0x00010001, 04, 01, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq1,0x00010001, AA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags1,0x00010001, 00, 01, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq1,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags1,0x00010001, 00, 01, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq1,0x00010001, FA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1001,0x00010001, 4F, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1001,0x00010001, 5E, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags1,0x00010001, 00, 01, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq1,0x00010001, F4, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1001,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1001,0x00010001, 93, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags1,0x00010001, 00, 01, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq1,0x00010001, E2, 04, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1001,0x00010001, 38, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1001,0x00010001, F1, FB, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags1,0x00010001, 00, 01, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq1,0x00010001, D0, 07, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags1,0x00010001, 00, 01, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq1,0x00010001, 8E, 12, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1001,0x00010001, 25, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1001,0x00010001, 12, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags1,0x00010001, 00, 01, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq1,0x00010001, 40, 1F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1001,0x00010001, 25, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags1,0x00010001, 02, 01, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq1,0x00010001, 88, 13, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1001,0x00010001, 17, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags2,0x00010001, 04, 02, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq2,0x00010001, AA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags2,0x00010001, 04, 02, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq2,0x00010001, AA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags2,0x00010001, 00, 02, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq2,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags2,0x00010001, 00, 02, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq2,0x00010001, FA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1002,0x00010001, 4F, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1002,0x00010001, 5E, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags2,0x00010001, 00, 02, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq2,0x00010001, F4, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1002,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1002,0x00010001, 93, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags2,0x00010001, 00, 02, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq2,0x00010001, E2, 04, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1002,0x00010001, 38, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1002,0x00010001, F1, FB, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags2,0x00010001, 00, 02, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq2,0x00010001, D0, 07, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags2,0x00010001, 00, 02, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq2,0x00010001, 8E, 12, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1002,0x00010001, 25, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1002,0x00010001, 12, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags2,0x00010001, 00, 02, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq2,0x00010001, 40, 1F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1002,0x00010001, 25, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags2,0x00010001, 02, 02, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq2,0x00010001, 88, 13, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1002,0x00010001, 17, 01, 00, 00
 
[SoftEQ.PCAN3.AddReg]
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1,SystemName,,PCAN3
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ProfileName,,default int spk
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,SpeakerApplication,,InternalSpeaker
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ProfileName,,default_int_spk
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,SpeakerApplication,,InternalSpeaker
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Cancel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Channel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,NumBands,0x00010001, 0A, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolLeft,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolRight,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,DRCEnable,0x00010001, 01, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTime,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTimeInMS,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTime,0x00010001, 00, 14, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTimeInMS,0x00010001, 00, 14, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Threshold,0x00010001, 00, 00, 80, BF
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,LinearGain,0x00010001, 00, 00, 88, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxInputLevel,0x00010001, 00, 00, A8, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxOutputLevel,0x00010001, 00, 98, 99, BE
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags1,0x00010001, 04, 01, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq1,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags1,0x00010001, 04, 01, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq1,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags1,0x00010001, 00, 01, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq1,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags1,0x00010001, 00, 01, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq1,0x00010001, C2, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1001,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1001,0x00010001, CB, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags1,0x00010001, 00, 01, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq1,0x00010001, E2, 04, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1001,0x00010001, 1C, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1001,0x00010001, F9, FD, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags1,0x00010001, 00, 01, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq1,0x00010001, 7E, 04, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1001,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1001,0x00010001, 50, FD, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags1,0x00010001, 00, 01, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq1,0x00010001, 40, 06, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1001,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1001,0x00010001, CB, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags1,0x00010001, 00, 01, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq1,0x00010001, 66, 08, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1001,0x00010001, 78, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags1,0x00010001, 00, 01, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq1,0x00010001, 38, 18, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags1,0x00010001, 02, 01, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq1,0x00010001, 70, 17, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1001,0x00010001, 12, 02, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags2,0x00010001, 04, 02, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq2,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags2,0x00010001, 04, 02, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq2,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags2,0x00010001, 00, 02, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq2,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags2,0x00010001, 00, 02, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq2,0x00010001, C2, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1002,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1002,0x00010001, CB, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags2,0x00010001, 00, 02, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq2,0x00010001, E2, 04, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1002,0x00010001, 1C, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1002,0x00010001, F9, FD, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags2,0x00010001, 00, 02, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq2,0x00010001, 7E, 04, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1002,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1002,0x00010001, 50, FD, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags2,0x00010001, 00, 02, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq2,0x00010001, 40, 06, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1002,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1002,0x00010001, CB, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags2,0x00010001, 00, 02, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq2,0x00010001, 66, 08, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1002,0x00010001, 78, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags2,0x00010001, 00, 02, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq2,0x00010001, 38, 18, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags2,0x00010001, 02, 02, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq2,0x00010001, 70, 17, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1002,0x00010001, 12, 02, 00, 00
 
[SoftEQ.CRML3.AddReg]
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1,SystemName,,CRML3
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ProfileName,,default int spk
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,SpeakerApplication,,InternalSpeaker
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Cancel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Channel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,NumBands,0x00010001, 0A, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolLeft,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolRight,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,DRCEnable,0x00010001, 01, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTime,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTimeInMS,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTime,0x00010001, 35, 0C, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTimeInMS,0x00010001, 35, 0C, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Threshold,0x00010001, 00, 00, 80, BF
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,LinearGain,0x00010001, 00, 00, 40, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxInputLevel,0x00010001, 00, 00, 90, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxOutputLevel,0x00010001, 00, 98, 99, BE
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags1,0x00010001, 04, 01, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq1,0x00010001, 8C, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags1,0x00010001, 04, 01, 03, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq1,0x00010001, 8C, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags1,0x00010001, 00, 01, 05, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq1,0x00010001, 2C, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1001,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags1,0x00010001, 00, 01, 09, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq1,0x00010001, C2, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1001,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1001,0x00010001, A3, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags1,0x00010001, 00, 01, 11, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq1,0x00010001, 84, 03, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1001,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1001,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags1,0x00010001, 00, 01, 21, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq1,0x00010001, 14, 05, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1001,0x00010001, 51, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1001,0x00010001, 1F, FF, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags1,0x00010001, 00, 01, 41, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq1,0x00010001, E2, 04, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1001,0x00010001, 19, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1001,0x00010001, 93, FC, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags1,0x00010001, 00, 01, 81, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq1,0x00010001, C4, 09, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1001,0x00010001, 1E, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags1,0x00010001, 00, 01, 01, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq1,0x00010001, B8, 0B, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags1,0x00010001, 02, 01, 01, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq1,0x00010001, 94, 11, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1001,0x00010001, 32, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1001,0x00010001, DC, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags2,0x00010001, 04, 02, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq2,0x00010001, 8C, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags2,0x00010001, 04, 02, 03, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq2,0x00010001, 8C, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags2,0x00010001, 00, 02, 05, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq2,0x00010001, 2C, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1002,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags2,0x00010001, 00, 02, 09, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq2,0x00010001, C2, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1002,0x00010001, 7D, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1002,0x00010001, A3, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags2,0x00010001, 00, 02, 11, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq2,0x00010001, 84, 03, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1002,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1002,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags2,0x00010001, 00, 02, 21, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq2,0x00010001, 14, 05, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1002,0x00010001, 51, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1002,0x00010001, 1F, FF, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags2,0x00010001, 00, 02, 41, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq2,0x00010001, E2, 04, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1002,0x00010001, 19, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1002,0x00010001, 93, FC, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags2,0x00010001, 00, 02, 81, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq2,0x00010001, C4, 09, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1002,0x00010001, 1E, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags2,0x00010001, 00, 02, 01, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq2,0x00010001, B8, 0B, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags2,0x00010001, 02, 02, 01, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq2,0x00010001, 94, 11, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1002,0x00010001, 32, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1002,0x00010001, DC, 00, 00, 00
 
[SoftEQ.KNDO.AddReg]
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1,SystemName,,KNDO
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ProfileName,,default int spk
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,SpeakerApplication,,InternalSpeaker
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Cancel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Channel,0x00010001, 00, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,NumBands,0x00010001, 0A, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolLeft,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ClippingCtrlVolRight,0x00010001, FF, 7F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,DRCEnable,0x00010001, 01, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTime,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,AttackTimeInMS,0x00010001, 14, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTime,0x00010001, 00, 05, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,ReleaseTimeInMS,0x00010001, 00, 05, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,Threshold,0x00010001, 00, 00, 80, BF
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,LinearGain,0x00010001, 00, 00, 70, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxInputLevel,0x00010001, 00, 00, 90, 40
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1,MaxOutputLevel,0x00010001, 00, 98, 99, BE
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags1,0x00010001, 04, 01, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq1,0x00010001, AA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags1,0x00010001, 04, 01, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq1,0x00010001, AA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1001,0x00010001, 32, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags1,0x00010001, 00, 01, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq1,0x00010001, E6, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1001,0x00010001, 2C, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags1,0x00010001, 00, 01, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq1,0x00010001, EE, 02, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1001,0x00010001, 25, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1001,0x00010001, 04, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags1,0x00010001, 00, 01, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq1,0x00010001, 90, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1001,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1001,0x00010001, C2, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags1,0x00010001, 00, 01, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq1,0x00010001, 84, 03, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1001,0x00010001, 44, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1001,0x00010001, 25, FF, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags1,0x00010001, 00, 01, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq1,0x00010001, C4, 09, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1001,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags1,0x00010001, 00, 01, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq1,0x00010001, A0, 0F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1001,0x00010001, 1C, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1001,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags1,0x00010001, 00, 01, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq1,0x00010001, 9C, 18, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1001,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1001,0x00010001, A3, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags1,0x00010001, 02, 01, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq1,0x00010001, 40, 1F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1001,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1001,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Flags2,0x00010001, 04, 02, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Freq2,0x00010001, AA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band1,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Flags2,0x00010001, 04, 02, 02, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Freq2,0x00010001, AA, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,BWx1002,0x00010001, 32, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band2,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Flags2,0x00010001, 00, 02, 04, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Freq2,0x00010001, E6, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band3,Gainx1002,0x00010001, 2C, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Flags2,0x00010001, 00, 02, 08, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Freq2,0x00010001, EE, 02, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,BWx1002,0x00010001, 25, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band4,Gainx1002,0x00010001, 04, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Flags2,0x00010001, 00, 02, 10, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Freq2,0x00010001, 90, 01, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,BWx1002,0x00010001, 4B, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band5,Gainx1002,0x00010001, C2, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Flags2,0x00010001, 00, 02, 20, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Freq2,0x00010001, 84, 03, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,BWx1002,0x00010001, 44, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band6,Gainx1002,0x00010001, 25, FF, FF, FF
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Flags2,0x00010001, 00, 02, 40, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Freq2,0x00010001, C4, 09, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band7,Gainx1002,0x00010001, 22, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Flags2,0x00010001, 00, 02, 80, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Freq2,0x00010001, A0, 0F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,BWx1002,0x00010001, 1C, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band8,Gainx1002,0x00010001, 00, 00, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Flags2,0x00010001, 00, 02, 00, 01
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Freq2,0x00010001, 9C, 18, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,BWx1002,0x00010001, 96, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band9,Gainx1002,0x00010001, A3, 01, 00, 00
 
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Flags2,0x00010001, 02, 02, 00, 02
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Freq2,0x00010001, 40, 1F, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,BWx1002,0x00010001, 64, 00, 00, 00
HKLM, SYSTEM\CurrentControlSet\Control\Conexant\EQ\1\1\Band10,Gainx1002,0x00010001, 22, 01, 00, 00
 
[EffectsEQ.AddReg]
HKLM, Software\Conexant\SAEQ\1,SystemName,,"Effects EQ Profiles"

; Classical
HKLM, Software\Conexant\SAEQ\1\1,ProfileName,,Classical
HKLM, Software\Conexant\SAEQ\1\1,SpeakerApplication,,Playback
HKLM, Software\Conexant\SAEQ\1\1,Cancel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\1,Channel,0x00010001,09,00,00,00
HKLM, Software\Conexant\SAEQ\1\1,NumBands,0x00010001,0a,00,00,00
HKLM, Software\Conexant\SAEQ\1\1,ClippingCtrlVol,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\1,ClippingCtrlVolRight,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\1,ClippingCtrlVolLeft,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\1,LinearGain,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\1,DRCEnable,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\1,Threshold,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\1,MaxInputLevel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\1,MaxOutputLevel,0x00010001,00,00,c0,33
HKLM, Software\Conexant\SAEQ\1\1,AttackTime,0x00010001,a0,00,00,00
HKLM, Software\Conexant\SAEQ\1\1,ReleaseTime,0x00010001,00,05,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band1,Flags1,0x00010001,01,01,01,00
HKLM, Software\Conexant\SAEQ\1\1\Band1,Freq1,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band1,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band1,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band2,Flags1,0x00010001,00,01,02,00
HKLM, Software\Conexant\SAEQ\1\1\Band2,Freq1,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band2,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band2,Gainx1001,0x00010001,4e,02,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band3,Flags1,0x00010001,00,01,04,00
HKLM, Software\Conexant\SAEQ\1\1\Band3,Freq1,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band3,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band3,Gainx1001,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band4,Flags1,0x00010001,00,01,08,00
HKLM, Software\Conexant\SAEQ\1\1\Band4,Freq1,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band4,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band4,Gainx1001,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band5,Flags1,0x00010001,00,01,10,00
HKLM, Software\Conexant\SAEQ\1\1\Band5,Freq1,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band5,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band5,Gainx1001,0x00010001,5d,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\1\Band6,Flags1,0x00010001,00,01,20,00
HKLM, Software\Conexant\SAEQ\1\1\Band6,Freq1,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band6,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band6,Gainx1001,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band7,Flags1,0x00010001,00,01,40,00
HKLM, Software\Conexant\SAEQ\1\1\Band7,Freq1,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band7,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band7,Gainx1001,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band8,Flags1,0x00010001,00,01,80,00
HKLM, Software\Conexant\SAEQ\1\1\Band8,Freq1,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band8,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band8,Gainx1001,0x00010001,4e,02,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band9,Flags1,0x00010001,00,01,00,01
HKLM, Software\Conexant\SAEQ\1\1\Band9,Freq1,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band9,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band9,Gainx1001,0x00010001,25,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\1\Band10,Flags1,0x00010001,02,01,00,02
HKLM, Software\Conexant\SAEQ\1\1\Band10,Freq1,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band10,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band10,Gainx1001,0x00010001,18,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\1\Band1,Flags2,0x00010001,01,02,01,00
HKLM, Software\Conexant\SAEQ\1\1\Band1,Freq2,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band1,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band1,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band2,Flags2,0x00010001,00,02,02,00
HKLM, Software\Conexant\SAEQ\1\1\Band2,Freq2,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band2,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band2,Gainx1002,0x00010001,4e,02,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band3,Flags2,0x00010001,00,02,04,00
HKLM, Software\Conexant\SAEQ\1\1\Band3,Freq2,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band3,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band3,Gainx1002,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band4,Flags2,0x00010001,00,02,08,00
HKLM, Software\Conexant\SAEQ\1\1\Band4,Freq2,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band4,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band4,Gainx1002,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band5,Flags2,0x00010001,00,02,10,00
HKLM, Software\Conexant\SAEQ\1\1\Band5,Freq2,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band5,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band5,Gainx1002,0x00010001,5d,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\1\Band6,Flags2,0x00010001,00,02,20,00
HKLM, Software\Conexant\SAEQ\1\1\Band6,Freq2,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band6,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band6,Gainx1002,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band7,Flags2,0x00010001,00,02,40,00
HKLM, Software\Conexant\SAEQ\1\1\Band7,Freq2,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band7,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band7,Gainx1002,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band8,Flags2,0x00010001,00,02,80,00
HKLM, Software\Conexant\SAEQ\1\1\Band8,Freq2,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band8,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band8,Gainx1002,0x00010001,4e,02,00,00

HKLM, Software\Conexant\SAEQ\1\1\Band9,Flags2,0x00010001,00,02,00,01
HKLM, Software\Conexant\SAEQ\1\1\Band9,Freq2,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band9,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band9,Gainx1002,0x00010001,25,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\1\Band10,Flags2,0x00010001,02,02,00,02
HKLM, Software\Conexant\SAEQ\1\1\Band10,Freq2,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band10,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\1\Band10,Gainx1002,0x00010001,18,fe,ff,ff

; Dance
HKLM, Software\Conexant\SAEQ\1\2,ProfileName,,Dance
HKLM, Software\Conexant\SAEQ\1\2,SpeakerApplication,,Playback
HKLM, Software\Conexant\SAEQ\1\2,Cancel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\2,Channel,0x00010001,09,00,00,00
HKLM, Software\Conexant\SAEQ\1\2,NumBands,0x00010001,0a,00,00,00
HKLM, Software\Conexant\SAEQ\1\2,ClippingCtrlVol,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\2,ClippingCtrlVolRight,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\2,ClippingCtrlVolLeft,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\2,LinearGain,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\2,DRCEnable,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\2,Threshold,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\2,MaxInputLevel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\2,MaxOutputLevel,0x00010001,00,00,c0,33
HKLM, Software\Conexant\SAEQ\1\2,AttackTime,0x00010001,a0,00,00,00
HKLM, Software\Conexant\SAEQ\1\2,ReleaseTime,0x00010001,00,05,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band1,Flags1,0x00010001,01,01,01,00
HKLM, Software\Conexant\SAEQ\1\2\Band1,Freq1,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band1,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band1,Gainx1001,0x00010001,4e,02,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band2,Flags1,0x00010001,00,01,02,00
HKLM, Software\Conexant\SAEQ\1\2\Band2,Freq1,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band2,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band2,Gainx1001,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band3,Flags1,0x00010001,00,01,04,00
HKLM, Software\Conexant\SAEQ\1\2\Band3,Freq1,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band3,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band3,Gainx1001,0x00010001,12,02,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band4,Flags1,0x00010001,00,01,08,00
HKLM, Software\Conexant\SAEQ\1\2\Band4,Freq1,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band4,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band4,Gainx1001,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band5,Flags1,0x00010001,00,01,10,00
HKLM, Software\Conexant\SAEQ\1\2\Band5,Freq1,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band5,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band5,Gainx1001,0x00010001,a3,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\2\Band6,Flags1,0x00010001,00,01,20,00
HKLM, Software\Conexant\SAEQ\1\2\Band6,Freq1,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band6,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band6,Gainx1001,0x00010001,a3,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\2\Band7,Flags1,0x00010001,00,01,40,00
HKLM, Software\Conexant\SAEQ\1\2\Band7,Freq1,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band7,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band7,Gainx1001,0x00010001,12,02,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band8,Flags1,0x00010001,00,01,80,00
HKLM, Software\Conexant\SAEQ\1\2\Band8,Freq1,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band8,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band8,Gainx1001,0x00010001,f7,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\2\Band9,Flags1,0x00010001,00,01,00,01
HKLM, Software\Conexant\SAEQ\1\2\Band9,Freq1,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band9,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band9,Gainx1001,0x00010001,78,00,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band10,Flags1,0x00010001,02,01,00,02
HKLM, Software\Conexant\SAEQ\1\2\Band10,Freq1,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band10,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band10,Gainx1001,0x00010001,fa,00,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band1,Flags2,0x00010001,01,02,01,00
HKLM, Software\Conexant\SAEQ\1\2\Band1,Freq2,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band1,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band1,Gainx1002,0x00010001,4e,02,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band2,Flags2,0x00010001,00,02,02,00
HKLM, Software\Conexant\SAEQ\1\2\Band2,Freq2,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band2,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band2,Gainx1002,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band3,Flags2,0x00010001,00,02,04,00
HKLM, Software\Conexant\SAEQ\1\2\Band3,Freq2,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band3,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band3,Gainx1002,0x00010001,12,02,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band4,Flags2,0x00010001,00,02,08,00
HKLM, Software\Conexant\SAEQ\1\2\Band4,Freq2,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band4,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band4,Gainx1002,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band5,Flags2,0x00010001,00,02,10,00
HKLM, Software\Conexant\SAEQ\1\2\Band5,Freq2,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band5,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band5,Gainx1002,0x00010001,a3,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\2\Band6,Flags2,0x00010001,00,02,20,00
HKLM, Software\Conexant\SAEQ\1\2\Band6,Freq2,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band6,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band6,Gainx1002,0x00010001,a3,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\2\Band7,Flags2,0x00010001,00,02,40,00
HKLM, Software\Conexant\SAEQ\1\2\Band7,Freq2,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band7,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band7,Gainx1002,0x00010001,12,02,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band8,Flags2,0x00010001,00,02,80,00
HKLM, Software\Conexant\SAEQ\1\2\Band8,Freq2,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band8,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band8,Gainx1002,0x00010001,f7,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\2\Band9,Flags2,0x00010001,00,02,00,01
HKLM, Software\Conexant\SAEQ\1\2\Band9,Freq2,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band9,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band9,Gainx1002,0x00010001,78,00,00,00

HKLM, Software\Conexant\SAEQ\1\2\Band10,Flags2,0x00010001,02,02,00,02
HKLM, Software\Conexant\SAEQ\1\2\Band10,Freq2,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band10,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\2\Band10,Gainx1002,0x00010001,fa,00,00,00

; Jazz
HKLM, Software\Conexant\SAEQ\1\3,ProfileName,,Jazz
HKLM, Software\Conexant\SAEQ\1\3,SpeakerApplication,,Playback
HKLM, Software\Conexant\SAEQ\1\3,Cancel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\3,Channel,0x00010001,09,00,00,00
HKLM, Software\Conexant\SAEQ\1\3,NumBands,0x00010001,0a,00,00,00
HKLM, Software\Conexant\SAEQ\1\3,ClippingCtrlVol,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\3,ClippingCtrlVolRight,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\3,ClippingCtrlVolLeft,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\3,LinearGain,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\3,DRCEnable,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\3,Threshold,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\3,MaxInputLevel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\3,MaxOutputLevel,0x00010001,00,00,c0,33
HKLM, Software\Conexant\SAEQ\1\3,AttackTime,0x00010001,a0,00,00,00
HKLM, Software\Conexant\SAEQ\1\3,ReleaseTime,0x00010001,00,05,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band1,Flags1,0x00010001,01,01,01,00
HKLM, Software\Conexant\SAEQ\1\3\Band1,Freq1,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band1,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band1,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band2,Flags1,0x00010001,00,01,02,00
HKLM, Software\Conexant\SAEQ\1\3\Band2,Freq1,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band2,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band2,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band3,Flags1,0x00010001,00,01,04,00
HKLM, Software\Conexant\SAEQ\1\3\Band3,Freq1,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band3,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band3,Gainx1001,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band4,Flags1,0x00010001,00,01,08,00
HKLM, Software\Conexant\SAEQ\1\3\Band4,Freq1,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band4,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band4,Gainx1001,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band5,Flags1,0x00010001,00,01,10,00
HKLM, Software\Conexant\SAEQ\1\3\Band5,Freq1,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band5,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band5,Gainx1001,0x00010001,b1,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\3\Band6,Flags1,0x00010001,00,01,20,00
HKLM, Software\Conexant\SAEQ\1\3\Band6,Freq1,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band6,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band6,Gainx1001,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band7,Flags1,0x00010001,00,01,40,00
HKLM, Software\Conexant\SAEQ\1\3\Band7,Freq1,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band7,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band7,Gainx1001,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band8,Flags1,0x00010001,00,01,80,00
HKLM, Software\Conexant\SAEQ\1\3\Band8,Freq1,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band8,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band8,Gainx1001,0x00010001,df,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\3\Band9,Flags1,0x00010001,00,01,00,01
HKLM, Software\Conexant\SAEQ\1\3\Band9,Freq1,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band9,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band9,Gainx1001,0x00010001,df,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\3\Band10,Flags1,0x00010001,02,01,00,02
HKLM, Software\Conexant\SAEQ\1\3\Band10,Freq1,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band10,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band10,Gainx1001,0x00010001,f7,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\3\Band1,Flags2,0x00010001,01,02,01,00
HKLM, Software\Conexant\SAEQ\1\3\Band1,Freq2,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band1,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band1,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band2,Flags2,0x00010001,00,02,02,00
HKLM, Software\Conexant\SAEQ\1\3\Band2,Freq2,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band2,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band2,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band3,Flags2,0x00010001,00,02,04,00
HKLM, Software\Conexant\SAEQ\1\3\Band3,Freq2,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band3,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band3,Gainx1002,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band4,Flags2,0x00010001,00,02,08,00
HKLM, Software\Conexant\SAEQ\1\3\Band4,Freq2,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band4,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band4,Gainx1002,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band5,Flags2,0x00010001,00,02,10,00
HKLM, Software\Conexant\SAEQ\1\3\Band5,Freq2,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band5,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band5,Gainx1002,0x00010001,b1,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\3\Band6,Flags2,0x00010001,00,02,20,00
HKLM, Software\Conexant\SAEQ\1\3\Band6,Freq2,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band6,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band6,Gainx1002,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band7,Flags2,0x00010001,00,02,40,00
HKLM, Software\Conexant\SAEQ\1\3\Band7,Freq2,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band7,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band7,Gainx1002,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\3\Band8,Flags2,0x00010001,00,02,80,00
HKLM, Software\Conexant\SAEQ\1\3\Band8,Freq2,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band8,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band8,Gainx1002,0x00010001,df,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\3\Band9,Flags2,0x00010001,00,02,00,01
HKLM, Software\Conexant\SAEQ\1\3\Band9,Freq2,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band9,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band9,Gainx1002,0x00010001,df,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\3\Band10,Flags2,0x00010001,02,02,00,02
HKLM, Software\Conexant\SAEQ\1\3\Band10,Freq2,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band10,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\3\Band10,Gainx1002,0x00010001,f7,ff,ff,ff

; Concert/Pop/Rock
HKLM, Software\Conexant\SAEQ\1\4,ProfileName,,Concert/Pop/Rock
HKLM, Software\Conexant\SAEQ\1\4,SpeakerApplication,,Playback
HKLM, Software\Conexant\SAEQ\1\4,Cancel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\4,Channel,0x00010001,09,00,00,00
HKLM, Software\Conexant\SAEQ\1\4,NumBands,0x00010001,0a,00,00,00
HKLM, Software\Conexant\SAEQ\1\4,ClippingCtrlVol,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\4,ClippingCtrlVolRight,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\4,ClippingCtrlVolLeft,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\4,LinearGain,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\4,DRCEnable,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\4,Threshold,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\4,MaxInputLevel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\4,MaxOutputLevel,0x00010001,00,00,c0,33
HKLM, Software\Conexant\SAEQ\1\4,AttackTime,0x00010001,a0,00,00,00
HKLM, Software\Conexant\SAEQ\1\4,ReleaseTime,0x00010001,00,05,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band1,Flags1,0x00010001,01,01,01,00
HKLM, Software\Conexant\SAEQ\1\4\Band1,Freq1,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band1,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band1,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band2,Flags1,0x00010001,00,01,02,00
HKLM, Software\Conexant\SAEQ\1\4\Band2,Freq1,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band2,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band2,Gainx1001,0x00010001,b1,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\4\Band3,Flags1,0x00010001,00,01,04,00
HKLM, Software\Conexant\SAEQ\1\4\Band3,Freq1,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band3,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band3,Gainx1001,0x00010001,f7,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\4\Band4,Flags1,0x00010001,00,01,08,00
HKLM, Software\Conexant\SAEQ\1\4\Band4,Freq1,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band4,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band4,Gainx1001,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band5,Flags1,0x00010001,00,01,10,00
HKLM, Software\Conexant\SAEQ\1\4\Band5,Freq1,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band5,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band5,Gainx1001,0x00010001,bb,00,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band6,Flags1,0x00010001,00,01,20,00
HKLM, Software\Conexant\SAEQ\1\4\Band6,Freq1,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band6,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band6,Gainx1001,0x00010001,df,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\4\Band7,Flags1,0x00010001,00,01,40,00
HKLM, Software\Conexant\SAEQ\1\4\Band7,Freq1,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band7,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band7,Gainx1001,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band8,Flags1,0x00010001,00,01,80,00
HKLM, Software\Conexant\SAEQ\1\4\Band8,Freq1,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band8,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band8,Gainx1001,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band9,Flags1,0x00010001,00,01,00,01
HKLM, Software\Conexant\SAEQ\1\4\Band9,Freq1,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band9,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band9,Gainx1001,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band10,Flags1,0x00010001,02,01,00,02
HKLM, Software\Conexant\SAEQ\1\4\Band10,Freq1,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band10,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band10,Gainx1001,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band1,Flags2,0x00010001,01,02,01,00
HKLM, Software\Conexant\SAEQ\1\4\Band1,Freq2,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band1,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band1,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band2,Flags2,0x00010001,00,02,02,00
HKLM, Software\Conexant\SAEQ\1\4\Band2,Freq2,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band2,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band2,Gainx1002,0x00010001,b1,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\4\Band3,Flags2,0x00010001,00,02,04,00
HKLM, Software\Conexant\SAEQ\1\4\Band3,Freq2,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band3,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band3,Gainx1002,0x00010001,f7,ff,ff,ff

HKLM, Software\Conexant\SAEQ\1\4\Band4,Flags2,0x00010001,00,02,08,00
HKLM, Software\Conexant\SAEQ\1\4\Band4,Freq2,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band4,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band4,Gainx1002,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band5,Flags2,0x00010001,00,02,10,00
HKLM, Software\Conexant\SAEQ\1\4\Band5,Freq2,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band5,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band5,Gainx1002,0x00010001,bb,00,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band6,Flags2,0x00010001,00,02,20,00
HKLM, Software\Conexant\SAEQ\1\4\Band6,Freq2,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band6,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band6,Gainx1002,0x00010001,df,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\4\Band7,Flags2,0x00010001,00,02,40,00
HKLM, Software\Conexant\SAEQ\1\4\Band7,Freq2,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band7,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band7,Gainx1002,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band8,Flags2,0x00010001,00,02,80,00
HKLM, Software\Conexant\SAEQ\1\4\Band8,Freq2,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band8,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band8,Gainx1002,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band9,Flags2,0x00010001,00,02,00,01
HKLM, Software\Conexant\SAEQ\1\4\Band9,Freq2,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band9,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band9,Gainx1002,0x00010001,40,01,00,00

HKLM, Software\Conexant\SAEQ\1\4\Band10,Flags2,0x00010001,02,02,00,02
HKLM, Software\Conexant\SAEQ\1\4\Band10,Freq2,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band10,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\4\Band10,Gainx1002,0x00010001,cb,01,00,00

; Normal (flat)
HKLM, Software\Conexant\SAEQ\1\5,ProfileName,,Normal
HKLM, Software\Conexant\SAEQ\1\5,SpeakerApplication,,Playback
HKLM, Software\Conexant\SAEQ\1\5,Cancel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\5,Channel,0x00010001,09,00,00,00
HKLM, Software\Conexant\SAEQ\1\5,NumBands,0x00010001,0a,00,00,00
HKLM, Software\Conexant\SAEQ\1\5,ClippingCtrlVol,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\5,ClippingCtrlVolRight,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\5,ClippingCtrlVolLeft,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\5,LinearGain,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\5,DRCEnable,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\5,Threshold,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\5,MaxInputLevel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\5,MaxOutputLevel,0x00010001,00,00,c0,33
HKLM, Software\Conexant\SAEQ\1\5,AttackTime,0x00010001,a0,00,00,00
HKLM, Software\Conexant\SAEQ\1\5,ReleaseTime,0x00010001,00,05,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band1,Flags1,0x00010001,01,01,01,00
HKLM, Software\Conexant\SAEQ\1\5\Band1,Freq1,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band1,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band1,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band2,Flags1,0x00010001,00,01,02,00
HKLM, Software\Conexant\SAEQ\1\5\Band2,Freq1,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band2,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band2,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band3,Flags1,0x00010001,00,01,04,00
HKLM, Software\Conexant\SAEQ\1\5\Band3,Freq1,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band3,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band3,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band4,Flags1,0x00010001,00,01,08,00
HKLM, Software\Conexant\SAEQ\1\5\Band4,Freq1,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band4,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band4,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band5,Flags1,0x00010001,00,01,10,00
HKLM, Software\Conexant\SAEQ\1\5\Band5,Freq1,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band5,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band5,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band6,Flags1,0x00010001,00,01,20,00
HKLM, Software\Conexant\SAEQ\1\5\Band6,Freq1,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band6,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band6,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band7,Flags1,0x00010001,00,01,40,00
HKLM, Software\Conexant\SAEQ\1\5\Band7,Freq1,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band7,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band7,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band8,Flags1,0x00010001,00,01,80,00
HKLM, Software\Conexant\SAEQ\1\5\Band8,Freq1,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band8,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band8,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band9,Flags1,0x00010001,00,01,00,01
HKLM, Software\Conexant\SAEQ\1\5\Band9,Freq1,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band9,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band9,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band10,Flags1,0x00010001,02,01,00,02
HKLM, Software\Conexant\SAEQ\1\5\Band10,Freq1,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band10,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band10,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band1,Flags2,0x00010001,01,02,01,00
HKLM, Software\Conexant\SAEQ\1\5\Band1,Freq2,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band1,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band1,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band2,Flags2,0x00010001,00,02,02,00
HKLM, Software\Conexant\SAEQ\1\5\Band2,Freq2,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band2,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band2,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band3,Flags2,0x00010001,00,02,04,00
HKLM, Software\Conexant\SAEQ\1\5\Band3,Freq2,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band3,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band3,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band4,Flags2,0x00010001,00,02,08,00
HKLM, Software\Conexant\SAEQ\1\5\Band4,Freq2,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band4,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band4,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band5,Flags2,0x00010001,00,02,10,00
HKLM, Software\Conexant\SAEQ\1\5\Band5,Freq2,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band5,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band5,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band6,Flags2,0x00010001,00,02,20,00
HKLM, Software\Conexant\SAEQ\1\5\Band6,Freq2,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band6,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band6,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band7,Flags2,0x00010001,00,02,40,00
HKLM, Software\Conexant\SAEQ\1\5\Band7,Freq2,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band7,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band7,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band8,Flags2,0x00010001,00,02,80,00
HKLM, Software\Conexant\SAEQ\1\5\Band8,Freq2,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band8,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band8,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band9,Flags2,0x00010001,00,02,00,01
HKLM, Software\Conexant\SAEQ\1\5\Band9,Freq2,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band9,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band9,Gainx1002,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\5\Band10,Flags2,0x00010001,02,02,00,02
HKLM, Software\Conexant\SAEQ\1\5\Band10,Freq2,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band10,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\5\Band10,Gainx1002,0x00010001,00,00,00,00

; Voice
HKLM, Software\Conexant\SAEQ\1\6,ProfileName,,Voice
HKLM, Software\Conexant\SAEQ\1\6,SpeakerApplication,,Playback
HKLM, Software\Conexant\SAEQ\1\6,Cancel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\6,Channel,0x00010001,09,00,00,00
HKLM, Software\Conexant\SAEQ\1\6,NumBands,0x00010001,0a,00,00,00
HKLM, Software\Conexant\SAEQ\1\6,ClippingCtrlVol,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\6,ClippingCtrlVolRight,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\6,ClippingCtrlVolLeft,0x00010001,ff,7f,00,00
HKLM, Software\Conexant\SAEQ\1\6,LinearGain,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\6,DRCEnable,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\6,Threshold,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\6,MaxInputLevel,0x00010001,00,00,00,00
HKLM, Software\Conexant\SAEQ\1\6,MaxOutputLevel,0x00010001,00,00,c0,33
HKLM, Software\Conexant\SAEQ\1\6,AttackTime,0x00010001,a0,00,00,00
HKLM, Software\Conexant\SAEQ\1\6,ReleaseTime,0x00010001,00,05,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band1,Flags1,0x00010001,01,01,01,00
HKLM, Software\Conexant\SAEQ\1\6\Band1,Freq1,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band1,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band1,Gainx1001,0x00010001,b5,f6,ff,ff

HKLM, Software\Conexant\SAEQ\1\6\Band2,Flags1,0x00010001,00,01,02,00
HKLM, Software\Conexant\SAEQ\1\6\Band2,Freq1,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band2,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band2,Gainx1001,0x00010001,09,fd,ff,ff

HKLM, Software\Conexant\SAEQ\1\6\Band3,Flags1,0x00010001,00,01,04,00
HKLM, Software\Conexant\SAEQ\1\6\Band3,Freq1,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band3,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band3,Gainx1001,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band4,Flags1,0x00010001,00,01,08,00
HKLM, Software\Conexant\SAEQ\1\6\Band4,Freq1,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band4,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band4,Gainx1001,0x00010001,93,02,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band5,Flags1,0x00010001,00,01,10,00
HKLM, Software\Conexant\SAEQ\1\6\Band5,Freq1,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band5,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band5,Gainx1001,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band6,Flags1,0x00010001,00,01,20,00
HKLM, Software\Conexant\SAEQ\1\6\Band6,Freq1,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band6,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band6,Gainx1001,0x00010001,5d,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\6\Band7,Flags1,0x00010001,00,01,40,00
HKLM, Software\Conexant\SAEQ\1\6\Band7,Freq1,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band7,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band7,Gainx1001,0x00010001,4e,02,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band8,Flags1,0x00010001,00,01,80,00
HKLM, Software\Conexant\SAEQ\1\6\Band8,Freq1,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band8,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band8,Gainx1001,0x00010001,93,02,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band9,Flags1,0x00010001,00,01,00,01
HKLM, Software\Conexant\SAEQ\1\6\Band9,Freq1,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band9,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band9,Gainx1001,0x00010001,fa,00,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band10,Flags1,0x00010001,02,01,00,02
HKLM, Software\Conexant\SAEQ\1\6\Band10,Freq1,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band10,BWx1001,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band10,Gainx1001,0x00010001,00,00,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band1,Flags2,0x00010001,01,02,01,00
HKLM, Software\Conexant\SAEQ\1\6\Band1,Freq2,0x00010001,1f,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band1,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band1,Gainx1002,0x00010001,b5,f6,ff,ff

HKLM, Software\Conexant\SAEQ\1\6\Band2,Flags2,0x00010001,00,02,02,00
HKLM, Software\Conexant\SAEQ\1\6\Band2,Freq2,0x00010001,3e,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band2,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band2,Gainx1002,0x00010001,09,fd,ff,ff

HKLM, Software\Conexant\SAEQ\1\6\Band3,Flags2,0x00010001,00,02,04,00
HKLM, Software\Conexant\SAEQ\1\6\Band3,Freq2,0x00010001,7d,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band3,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band3,Gainx1002,0x00010001,cb,01,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band4,Flags2,0x00010001,00,02,08,00
HKLM, Software\Conexant\SAEQ\1\6\Band4,Freq2,0x00010001,fa,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band4,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band4,Gainx1002,0x00010001,93,02,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band5,Flags2,0x00010001,00,02,10,00
HKLM, Software\Conexant\SAEQ\1\6\Band5,Freq2,0x00010001,f4,01,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band5,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band5,Gainx1002,0x00010001,86,01,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band6,Flags2,0x00010001,00,02,20,00
HKLM, Software\Conexant\SAEQ\1\6\Band6,Freq2,0x00010001,e8,03,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band6,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band6,Gainx1002,0x00010001,5d,fe,ff,ff

HKLM, Software\Conexant\SAEQ\1\6\Band7,Flags2,0x00010001,00,02,40,00
HKLM, Software\Conexant\SAEQ\1\6\Band7,Freq2,0x00010001,d0,07,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band7,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band7,Gainx1002,0x00010001,4e,02,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band8,Flags2,0x00010001,00,02,80,00
HKLM, Software\Conexant\SAEQ\1\6\Band8,Freq2,0x00010001,a0,0f,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band8,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band8,Gainx1002,0x00010001,93,02,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band9,Flags2,0x00010001,00,02,00,01
HKLM, Software\Conexant\SAEQ\1\6\Band9,Freq2,0x00010001,40,1f,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band9,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band9,Gainx1002,0x00010001,fa,00,00,00

HKLM, Software\Conexant\SAEQ\1\6\Band10,Flags2,0x00010001,02,02,00,02
HKLM, Software\Conexant\SAEQ\1\6\Band10,Freq2,0x00010001,80,3e,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band10,BWx1002,0x00010001,64,00,00,00
HKLM, Software\Conexant\SAEQ\1\6\Band10,Gainx1002,0x00010001,00,00,00,00

;; Settings for system effect begins
;;
;; All FX\\0 entries in the same grouping
;;
[RenderSysFx.AddReg]
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
;;HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
HKR,"FX\\0",%PKEY_FX_PreMixClsid%,,%FX_PREMIX_CLSID%
HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_ANY%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
 
[RenderSPKSysFx.AddReg]
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
;;HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
HKR,"FX\\0",%PKEY_FX_PreMixClsid%,,%FX_PREMIX_CLSID%
HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0010
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0001
HKR,"FX\\0",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_SPEAKER%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_SPEAKER%
HKR,"EP\\0", %PKEY_Endpoint_ID%, %REG_DWORD%, 0x0010
HKR,"EP\\0",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[RenderHPSysFx.AddReg]
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
;;HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
HKR,"FX\\0",%PKEY_FX_PreMixClsid%,,%FX_PREMIX_CLSID%
HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0050
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0001
HKR,"FX\\0",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_HEADPHONES%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_HEADPHONES%
HKR,"EP\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0050
HKR,"EP\\0",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[RenderSPDIFSysFx.AddReg]
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
;;HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
HKR,"FX\\0",%PKEY_FX_PreMixClsid%,,%FX_PREMIX_CLSID%
HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0020
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0001
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_SPDIF_INTERFACE%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_SPDIF_INTERFACE%
HKR,"EP\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0020
HKR,"EP\\0",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[CaptureMicSysFx.AddReg]
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE%
 
HKR,"FX\\1",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\1",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\1",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\1", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%
HKR,"EP\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\1",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[CaptureMicSysFxCMC.AddReg] ;classicmode collection
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE%
HKR,"EP\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\0",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
HKR,"EP\\0",%PKEY_Endpoint_Name% ,,"Internal Microphone"
HKR,"EP\\0",%PKEY_Device_Type%, %REG_DWORD%, 0x000F
 
HKR,"FX\\1",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\1",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\1",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\1", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%
HKR,"EP\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\1",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[CaptureMicSysFxADC.AddReg] ;analog digital collection
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE%
HKR,"EP\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\0",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
HKR,"EP\\0",%PKEY_Endpoint_Name% ,,"External Microphone"
 
HKR,"FX\\1",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\1",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\1",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\1", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%
HKR,"EP\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\1",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[CaptureMicSysFxADC1.AddReg] ;analog digital collection 2
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE%
HKR,"EP\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\0",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
HKR,"EP\\0",%PKEY_Endpoint_Name% ,,"Docking Microphone"
 
HKR,"FX\\1",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\1",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\1",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\1", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%
HKR,"EP\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\1",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[CaptureMicSysFxDC.AddReg]
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE%
HKR,"EP\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\0",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
HKR,"EP\\0",%PKEY_Endpoint_Name% ,,"Internal Microphone"
 
HKR,"FX\\1",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\1",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\1",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\1",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_BEAMFORMING%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_LFX_AEC%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_Endpoint_Enable_GFX%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_AudioEndpoint_Disable_SysFx%, %REG_DWORD%, 0x0000
HKR,"FX\\1",%PKEY_SYSFX_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\1", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_MICROPHONE_ARRAY%
HKR,"EP\\1",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0030
HKR,"EP\\1",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[CaptureLineinSysFx.AddReg]
HKR,"FX\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0040
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_LINE_CONNECTOR%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
HKR,"EP\\0",%PKEY_AudioEndpoint_Association%,,%KSNODETYPE_LINE_CONNECTOR%
HKR,"EP\\0",%PKEY_Endpoint_ID%, %REG_DWORD%, 0x0040 
HKR,"EP\\0",%PKEY_AudioEndpoint_Supports_EventDriven_Mode%,%REG_DWORD%,0x00000001
 
[CaptureSysFx.AddReg]
HKR,"FX\\0",%PKEY_DisplayName%,,%SYSFX_FriendlyName%
HKR,"FX\\0",%PKEY_SYSFX_PreMixClsid%,,%SYSFX_PREMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_PostMixClsid%,,%SYSFX_POSTMIX_CLSID%
;;HKR,"FX\\0",%PKEY_SYSFX_UiClsid%,,%SYSFX_UI_CLSID%
;;HKR,"FX\\0",%PKEY_FX_UiClsid%,,%FX_UI_CLSID%
HKR,"FX\\0",%PKEY_SYSFX_Association%,,%KSNODETYPE_ANY%  ; GUID NULL means install on all endpoints
                                                        ; supply a specific GUID to install on a particular bridge pin node type
;;
;; All EP\\0 entries in the same grouping
;;
;; Set default format to 48kHz, 16-bit, Stereo
;;
;;[OEMDefaultFormatOverride.AddReg]
;;HKR,"EP\\0", %PKEY_AudioEndpoint_Association%,,%KSNODETYPE_SPEAKER%
;;HKR,"EP\\0", %PKEY_AudioEngine_OEMFormat%, %REG_BINARY%, ;;41,00,8C,70,28,00,00,00,FE,FF,02,00,80,BB,00,00,00,EE,02,00,04,00,10,00,16,00,10,00,03,00,00,00,01,00,00,00,00,00,10,00,80,00,00,AA,00,38,9B,71
 
;;
;; Copy custom SYSFX and property page
;;
[SfxFx.CopyList]
CX64AQ17.dll
 
;;
;; Register custom SYSFX and property page
;;
[SfxFx.RegisterDlls]
11,,CX64AQ17.dll,1
 
;; Settings for system effect ends
 
[HdAudModel.SHINMV.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo

AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo

AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo

AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo

AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo

AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo

AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo

AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
 
;
; Independent microphone interfaces. Up to 5 are supported.
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
 
;
; Mic Array interfaces. By design, only one is supported
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
 
; Rear line out
[HdAudModel.NZMI1.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
 
;
; Independent microphone interfaces. Up to 5 are supported.
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
 
;
; Mic Array interfaces. By design, only one is supported
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
 
; Rear line out
[HdAudModel.NICO3.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
 
;
; Independent microphone interfaces. Up to 5 are supported.
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
 
;
; Mic Array interfaces. By design, only one is supported
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
 
; Rear line out
[HdAudModel.MOCA3.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
 
;
; Independent microphone interfaces. Up to 5 are supported.
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
 
;
; Mic Array interfaces. By design, only one is supported
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
 
; Rear line out
[HdAudModel.PCAN3.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
 
;
; Independent microphone interfaces. Up to 5 are supported.
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
 
;
; Mic Array interfaces. By design, only one is supported
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
 
; Rear line out
[HdAudModel.CRML3.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
 
;
; Independent microphone interfaces. Up to 5 are supported.
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
 
;
; Mic Array interfaces. By design, only one is supported
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
 
; Rear line out
[HdAudModel.KNDO.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_RearLineOutWave%, HdAudModel.RearLineOutWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineOutTopo%, HdAudModel.RearLineOutTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_RearLineInWave%, HdAudModel.RearLineInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_RearLineInTopo%, HdAudModel.RearLineInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_FrontPanelHeadphoneWave%, HdAudModel.FrontPanelHeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, HdAudModel.FrontPanelHeadphoneTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelMicWave%, HdAudModel.FrontPanelMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelMicTopo%, HdAudModel.FrontPanelMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCaptureWave%, HdAudModel.AnalogDigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCaptureTopo%, HdAudModel.AnalogDigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture1Wave%, HdAudModel.AnalogDigitalCapture1Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture1Topo%, HdAudModel.AnalogDigitalCapture1Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AnalogDigitalCapture2Wave%, HdAudModel.AnalogDigitalCapture2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AnalogDigitalCapture2Topo%, HdAudModel.AnalogDigitalCapture2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalCaptureWave%, HdAudModel.DigitalCaptureWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalCaptureTopo%, HdAudModel.DigitalCaptureTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutputWave%, HdAudModel.DigitalOutputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutputTopo%, HdAudModel.DigitalOutputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_DigitalOutput2Wave%, HdAudModel.DigitalOutput2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalOutput2Topo%, HdAudModel.DigitalOutput2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_DigitalInputWave%, HdAudModel.DigitalInputWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_DigitalInputTopo%, HdAudModel.DigitalInputTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_MicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_MicArrayTopo%, HdAudModel.MicArrayTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AuxInWave%, AzAudModel.AuxInWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_AuxInTopo%, AzAudModel.AuxInTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_FrontPanelHeadphoneWave%, AzAudModel.HeadphoneWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_FrontPanelHeadphoneTopo%, AzAudModel.HeadphoneTopo
 
;
; Independent microphone interfaces. Up to 5 are supported.
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicInWave%, HdAudModel.IndependentMicWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicInTopo%, HdAudModel.IndependentMicTopo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn2Wave%, HdAudModel.IndependentMic2Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn2Topo%, HdAudModel.IndependentMic2Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn3Wave%, HdAudModel.IndependentMic3Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn3Topo%, HdAudModel.IndependentMic3Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn4Wave%, HdAudModel.IndependentMic4Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn4Topo%, HdAudModel.IndependentMic4Topo
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicIn5Wave%, HdAudModel.IndependentMic5Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicIn5Topo%, HdAudModel.IndependentMic5Topo
 
;
; Mic Array interfaces. By design, only one is supported
;
 
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_eMicArrayWave%, HdAudModel.MicArrayWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_eMicArrayTopo%, HdAudModel.MicArrayTopo
 
; Rear line out
[HdAudModel.RearLineOutWave]
AddReg = HdAudModel.RearLineOutWave.AddReg

[HdAudModel.RearLineOutWave.AddReg]
HKR,,FriendlyName,,%RearLineOutWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

;HKR,,FriendlyName,,%RearLineOutDacName%
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

;IntHdAudGuid.RearLineOutDac
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidRearLineOutDac%,Name,,%RearLineOutDacName%
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidRearLineOutDac%,Display,1,00,00,00,00
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidDisableDigitalOutput%,Name,,%DisableDigitalOutputName%
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidDisableDigitalOutput%,Display,1,00,00,00,00
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidFrontHPOutDac%,Name,,%FrontHPOutDacName%
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidFrontHPOutDac%,Display,1,00,00,00,00
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidDigitalSpeaker%,Name,,%DigitalSpeakerName%
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidDigitalSpeaker%,Display,1,00,00,00,00
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidMicDockingSelect%,Name,,%MicDockingSelectName%
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidMicDockingSelect%,Display,1,00,00,00,00

HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidWaveOutMix%,Display,1,00,00,00
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HdAudGuidWaveOutMix%,Name,,%WaveOutMixName%
 
[HdAudModel.RearLineOutTopo]
AddReg = HdAudModel.RearLineOutTopo.AddReg, RenderSPKSysFx.AddReg

[HdAudModel.RearLineOutTopo.AddReg]
HKR,,FriendlyName,,%RearLineOutTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

; Rear line in

[HdAudModel.RearLineInWave]
AddReg = HdAudModel.RearLineInWave.AddReg

[HdAudModel.RearLineInWave.AddReg]
HKR,,FriendlyName,,%RearLineInWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

[HdAudModel.RearLineInTopo]
AddReg = HdAudModel.RearLineInTopo.AddReg, CaptureMicSysFx.AddReg

[HdAudModel.RearLineInTopo.AddReg]
HKR,,FriendlyName,,%RearLineInTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

; Front panel headphone

[HdAudModel.FrontPanelHeadphoneWave]
AddReg = HdAudModel.FrontPanelHeadphoneWave.AddReg

[HdAudModel.FrontPanelHeadphoneWave.AddReg]
HKR,,FriendlyName,,%FrontPanelHeadphoneWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

[HdAudModel.FrontPanelHeadphoneTopo]
AddReg = HdAudModel.FrontPanelHeadphoneTopo.AddReg, RenderHPSysFx.AddReg

[HdAudModel.FrontPanelHeadphoneTopo.AddReg]
HKR,,FriendlyName,,%FrontPanelHeadphoneTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

; Front panel mic

[HdAudModel.FrontPanelMicWave]
AddReg = HdAudModel.FrontPanelMicWave.AddReg

[HdAudModel.FrontPanelMicWave.AddReg]
HKR,,FriendlyName,,%FrontPanelMicWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

[HdAudModel.FrontPanelMicTopo]
AddReg = HdAudModel.FrontPanelMicTopo.AddReg, CaptureSysFx.AddReg

[HdAudModel.FrontPanelMicTopo.AddReg]
HKR,,FriendlyName,,%FrontPanelMicTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

; Digital output

[HdAudModel.DigitalOutputWave]
AddReg = HdAudModel.DigitalOutputWave.AddReg

[HdAudModel.DigitalOutputWave.AddReg]
HKR,,FriendlyName,,%DigitalOutputWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

[HdAudModel.DigitalOutputTopo]
AddReg = HdAudModel.DigitalOutputTopo.AddReg, RenderSPDIFSysFx.AddReg

[HdAudModel.DigitalOutputTopo.AddReg]
HKR,,FriendlyName,,%DigitalOutputTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

; Digital output 2
 
[HdAudModel.DigitalOutput2Wave]
AddReg = HdAudModel.DigitalOutput2Wave.AddReg
 
[HdAudModel.DigitalOutput2Wave.AddReg]
HKR,,FriendlyName,,%DigitalOutputWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
 
[HdAudModel.DigitalOutput2Topo]
AddReg = HdAudModel.DigitalOutput2Topo.AddReg, RenderSPDIFSysFx.AddReg
 
[HdAudModel.DigitalOutput2Topo.AddReg]
HKR,,FriendlyName,,%DigitalOutputTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
 
; Pebble Capture 1
 
[HdAudModel.AnalogDigitalCaptureWave]
AddReg = HdAudModel.AnalogDigitalCaptureWave.AddReg
 
[HdAudModel.AnalogDigitalCaptureWave.AddReg]
HKR,,FriendlyName,,%AnalogDigitalCaptureWaveName%
HKR,,CLSID,,%Proxy.CLSID%
 
[HdAudModel.AnalogDigitalCaptureTopo]
AddReg = HdAudModel.AnalogDigitalCaptureTopo.AddReg, CaptureMicSysFxADC.AddReg
 
[HdAudModel.AnalogDigitalCaptureTopo.AddReg]
HKR,,FriendlyName,,%AnalogDigitalCaptureTopoName%
HKR,,CLSID,,%Proxy.CLSID%
 
;Pebble Capture 2
 
[HdAudModel.AnalogDigitalCapture1Wave]
AddReg = HdAudModel.AnalogDigitalCapture1Wave.AddReg
 
[HdAudModel.AnalogDigitalCapture1Wave.AddReg]
HKR,,FriendlyName,,%AnalogDigitalCaptureWaveName%
HKR,,CLSID,,%Proxy.CLSID%
 
[HdAudModel.AnalogDigitalCapture1Topo]
AddReg = HdAudModel.AnalogDigitalCapture1Topo.AddReg, CaptureMicSysFxADC1.AddReg
 
[HdAudModel.AnalogDigitalCapture1Topo.AddReg]
HKR,,FriendlyName,,%AnalogDigitalCaptureTopoName%
HKR,,CLSID,,%Proxy.CLSID%
 
; Pebble Capture 3
 
[HdAudModel.AnalogDigitalCapture2Wave]
AddReg = HdAudModel.AnalogDigitalCapture2Wave.AddReg
 
[HdAudModel.AnalogDigitalCapture2Wave.AddReg]
HKR,,FriendlyName,,%AnalogDigitalCaptureWaveName%
HKR,,CLSID,,%Proxy.CLSID%
 
[HdAudModel.AnalogDigitalCapture2Topo]
AddReg = HdAudModel.AnalogDigitalCapture2Topo.AddReg, CaptureMicSysFxCMC.AddReg
 
[HdAudModel.AnalogDigitalCapture2Topo.AddReg]
HKR,,FriendlyName,,%AnalogDigitalCaptureTopoName%
HKR,,CLSID,,%Proxy.CLSID%
 
; Pebble Digital Capture 4 (internal digital mic)
 
[HdAudModel.DigitalCaptureWave]
AddReg = HdAudModel.DigitalCaptureWave.AddReg
 
[HdAudModel.DigitalCaptureWave.AddReg]
HKR,,FriendlyName,,%DigitalCaptureWaveName%
HKR,,CLSID,,%Proxy.CLSID%
 
[HdAudModel.DigitalCaptureTopo]
AddReg = HdAudModel.DigitalCaptureTopo.AddReg, CaptureMicSysFxDC.AddReg
 
[HdAudModel.DigitalCaptureTopo.AddReg]
HKR,,FriendlyName,,%DigitalCaptureTopoName%
HKR,,CLSID,,%Proxy.CLSID%
 
; Digital input

[HdAudModel.DigitalInputWave]
AddReg = HdAudModel.DigitalInputWave.AddReg

[HdAudModel.DigitalInputWave.AddReg]
HKR,,FriendlyName,,%DigitalInputWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

[HdAudModel.DigitalInputTopo]
AddReg = HdAudModel.DigitalInputTopo.AddReg

[HdAudModel.DigitalInputTopo.AddReg]
HKR,,FriendlyName,,%DigitalInputTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

; Microphone Array

[HdAudModel.MicArrayWave]
AddReg = HdAudModel.MicArrayWave.AddReg

[HdAudModel.MicArrayWave.AddReg]
HKR,,FriendlyName,,%MicArrayWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

[HdAudModel.MicArrayTopo]
AddReg = HdAudModel.MicArrayTopo.AddReg, CaptureSysFx.AddReg

[HdAudModel.MicArrayTopo.AddReg]
HKR,,FriendlyName,,%MicArrayTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

; Auxiliary Input

[AzAudModel.AuxInWave]
AddReg = AzAudModel.AuxInWave.AddReg

[AzAudModel.AuxInWave.AddReg]
HKR,,FriendlyName,,%AuxInWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

[AzAudModel.AuxInTopo]
AddReg = AzAudModel.AuxInTopo.AddReg, CaptureLineinSysFx.AddReg

[AzAudModel.AuxInTopo.AddReg]
HKR,,FriendlyName,,%AuxInTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%

; Headphone Output
 
[AzAudModel.HeadphoneWave]
AddReg = AzAudModel.HeadphoneWave.AddReg
 
[AzAudModel.HeadphoneWave.AddReg]
HKR,,FriendlyName,,%FrontPanelHeadphoneWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
 
[AzAudModel.HeadphoneTopo]
AddReg = RenderHPSysFx.AddReg
 
;
; Mic In Model & Add Reg. Up to 5 Instances supported
;
 
; 1st instance
[HdAudModel.IndependentMicWave]
AddReg = HdAudModel.IndependentMicWave.AddReg
[HdAudModel.IndependentMicWave.AddReg]
HKR,,FriendlyName,,%IndependentMicWaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
[HdAudModel.IndependentMicTopo]
AddReg = HdAudModel.IndependentMicTopo.AddReg, CaptureSysFx.AddReg
[HdAudModel.IndependentMicTopo.AddReg]
HKR,,FriendlyName,,%IndependentMicTopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
 
; 2nd instance of Mic In
[HdAudModel.IndependentMic2Wave]
AddReg = HdAudModel.IndependentMic2Wave.AddReg
[HdAudModel.IndependentMic2Wave.AddReg]
HKR,,FriendlyName,,%IndependentMic2WaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
[HdAudModel.IndependentMic2Topo]
AddReg = HdAudModel.IndependentMic2Topo.AddReg, CaptureSysFx.AddReg
[HdAudModel.IndependentMic2Topo.AddReg]
HKR,,FriendlyName,,%IndependentMic2TopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
 
; 3rd instance of Mic In
[HdAudModel.IndependentMic3Wave]
AddReg = HdAudModel.IndependentMic3Wave.AddReg
[HdAudModel.IndependentMic3Wave.AddReg]
HKR,,FriendlyName,,%IndependentMic3WaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
[HdAudModel.IndependentMic3Topo]
AddReg = HdAudModel.IndependentMic3Topo.AddReg, CaptureSysFx.AddReg
[HdAudModel.IndependentMic3Topo.AddReg]
HKR,,FriendlyName,,%IndependentMic3TopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
 
; 4th instance of Mic In
[HdAudModel.IndependentMic4Wave]
AddReg = HdAudModel.IndependentMic4Wave.AddReg
[HdAudModel.IndependentMic4Wave.AddReg]
HKR,,FriendlyName,,%IndependentMic4WaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
[HdAudModel.IndependentMic4Topo]
AddReg = HdAudModel.IndependentMic4Topo.AddReg, CaptureSysFx.AddReg
[HdAudModel.IndependentMic4Topo.AddReg]
HKR,,FriendlyName,,%IndependentMic4TopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
 
; 5th instance of Mic In
[HdAudModel.IndependentMic5Wave]
AddReg = HdAudModel.IndependentMic5Wave.AddReg
[HdAudModel.IndependentMic5Wave.AddReg]
HKR,,FriendlyName,,%IndependentMic5WaveDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
[HdAudModel.IndependentMic5Topo]
AddReg = HdAudModel.IndependentMic5Topo.AddReg, CaptureSysFx.AddReg
[HdAudModel.IndependentMic5Topo.AddReg]
HKR,,FriendlyName,,%IndependentMic5TopoDeviceName%
HKR,,CLSID,,%Proxy.CLSID%
 
;
; Microphone Array Model and AddReg. 1 Instance supported
;
 
[HdAudSecurity.AddReg]
; FILE_DEVICE_SOUND
HKR,,DeviceType,0x10001,0x0000001D
; SDDL_DEVOBJ_SYS_ALL_ADM_RWX_WORLD_RWX_RES_RWX
HKR,,Security,,"D:P(A;;GA;;;SY)(A;;GRGWGX;;;BA)(A;;GRGWGX;;;WD)(A;;GRGWGX;;;RC)"

[Strings]
CompanyName = "Conexant"
ProductName = "Conexant 20585 SmartAudio HD"
VersionInfo = "4.95.48.50"
DiskId1 = "Conexant 20585 SmartAudio HD Audio Driver Installation Disk"
HdAudioFunctionDriver.Pebble5071.DeviceDesc = "Conexant 20585 SmartAudio HD"
UAAFunctionDriverForHdAudio.SvcDesc = "Conexant UAA Function Driver for High Definition Audio Service"

;;use one name, we are not supporting dynamic subdevices
HDAudioOEMFriendlyName   = "Conexant 20585 SmartAudio HD"
RearLineOutWaveDeviceName =        "Conexant HD Audio output"
RearLineOutDacName =               "Conexant HD Audio line out"
RearLineInWaveDeviceName =         "Conexant HD Audio input"
RearMicInWaveDeviceName =          "Conexant HD Audio mic"
FrontPanelHeadphoneWaveDeviceName ="Conexant HD Audio headphone"
FrontHPOutDacName =                "Conexant HD Audio headphone"
FrontPanelMicWaveDeviceName =      "Conexant HD Audio mic"
DigitalOutputWaveDeviceName =      "Conexant HD Audio digital out"
DigitalInputWaveDeviceName =       "Conexant HD Audio digital in"
;MicArrayWaveDeviceName =           "Conexant HD Audio mic array"
AuxInWaveDeviceName =              "Conexant HD Audio aux in"
AnalogDigitalCaptureWaveName =     "Conexant HD Audio capture" 
DigitalCaptureWaveName =           "Conexant HD Audio capture" 
 
RearLineOutTopoDeviceName =        "Conexant HD Audio output mixer"
RearLineInTopoDeviceName =         "Conexant HD Audio input mixer"
RearMicInTopoDeviceName =          "Conexant HD Audio mic mixer"
FrontPanelHeadphoneTopoDeviceName ="Conexant HD Audio headphone mixer"
FrontPanelMicTopoDeviceName =      "Conexant HD Audio mic mixer"
DigitalOutputTopoDeviceName =      "Conexant HD Audio digital out mixer"
DigitalInputTopoDeviceName =       "Conexant HD Audio digital in mixer"
;MicArrayTopoDeviceName =           "Conexant HD Audio mic array mixer"
AuxInTopoDeviceName =              "Conexant HD Audio aux in mixer"
AnalogDigitalCaptureTopoName =     "Conexant HD Audio capture mixer" 
DigitalCaptureTopoName =           "Conexant HD Audio capture mixer" 
 
IndependentMicWaveDeviceName  = "Conexant HD Audio Microphone"
IndependentMicTopoDeviceName  = "Conexant HD Audio Microphone mixer"
IndependentMic2WaveDeviceName = "Conexant HD Audio Microphone 2"
IndependentMic2TopoDeviceName = "Conexant HD Audio Microphone 2 mixer"
IndependentMic3WaveDeviceName = "Conexant HD Audio Microphone 3"
IndependentMic3TopoDeviceName = "Conexant HD Audio Microphone 3 mixer"
IndependentMic4WaveDeviceName = "Conexant HD Audio Microphone 4"
IndependentMic4TopoDeviceName = "Conexant HD Audio Microphone 4 mixer"
IndependentMic5WaveDeviceName = "Conexant HD Audio Microphone 5"
IndependentMic5TopoDeviceName = "Conexant HD Audio Microphone 5 mixer"
 
MicArrayWaveDeviceName =        "Conexant HD Audio Microphone array"
MicArrayTopoDeviceName =        "Conexant HD Audio Microphone array mixer"
 
;;;RearLineOutWaveDeviceName =        "Conexant HD Audio"
;;;RearLineOutDacName =               "Conexant HD Audio"
;;;RearLineInWaveDeviceName =         "Conexant HD Audio"
;;;RearMicInWaveDeviceName =          "Conexant HD Audio"
;;;FrontPanelHeadphoneWaveDeviceName ="Conexant HD Audio"
;;;FrontHPOutDacName =                "Conexant HD Audio"
;;;FrontPanelMicWaveDeviceName =      "Conexant HD Audio"
;;;DigitalOutputWaveDeviceName =      "Conexant HD Audio"
;;;DigitalInputWaveDeviceName =       "Conexant HD Audio"
;;;MicArrayWaveDeviceName =           "Conexant HD Audio"
;;;AuxInWaveDeviceName =              "Conexant HD Audio"
 
;;;RearLineOutTopoDeviceName =        "Conexant HD Audio"
;;;RearLineInTopoDeviceName =         "Conexant HD Audio"
;;;RearMicInTopoDeviceName =          "Conexant HD Audio"
;;;FrontPanelHeadphoneTopoDeviceName ="Conexant HD Audio"
;;;FrontPanelMicTopoDeviceName =      "Conexant HD Audio"
;;;DigitalOutputTopoDeviceName =      "Conexant HD Audio"
;;;DigitalInputTopoDeviceName =       "Conexant HD Audio"
;;;MicArrayTopoDeviceName =           "Conexant HD Audio"
;;;AuxInTopoDeviceName =              "Conexant HD Audio"

DisableDigitalOutputName = "Disable Digital Output"
HdAudioDeviceDescription = "Conexant Pebble High Definition SmartAudio"
DigitalSpeakerName	 = "Digital Speaker"
MicDockingSelectName	= "Mic Docking Sel"
WaveOutMixName           = "WaveOut Mix"

KSNAME_RearLineOutWave = "RearLineOutWave" ; non-localizable
KSNAME_RearLineInWave = "RearLineInWave" ; non-localizable
KSNAME_FrontPanelHeadphoneWave ="FrontPanelHeadphoneWave" ; non-localizable
KSNAME_FrontPanelMicWave = "FrontPanelMicWave" ; non-localizable
KSNAME_DigitalOutputWave = "DigitalOutputWave" ; non-localizable
KSNAME_DigitalOutput2Wave = "DigitalOutput2Wave" ; non-localizable
KSNAME_DigitalInputWave = "DigitalInputWave" ; non-localizable
KSNAME_MicArrayWave = "MicArrayWave" ; non-localizable
KSNAME_AuxInWave = "AuxInputWave" ; non-localizable
KSNAME_AnalogDigitalCaptureWave = "AnalogDigitalCaptureWave" ; non-localizable
KSNAME_AnalogDigitalCapture1Wave = "AnalogDigitalCapture1Wave" ; non-localizable
KSNAME_AnalogDigitalCapture2Wave = "AnalogDigitalCapture2Wave" ; non-localizable
KSNAME_HeadphoneWave = "HeadphoneWave" ; non-localizable
KSNAME_DigitalCaptureWave = "DigitalCaptureWave" ; non-localizable

KSNAME_RearLineOutTopo = "RearLineOutTopo" ; non-localizable
KSNAME_RearLineInTopo = "RearLineInTopo" ; non-localizable
KSNAME_FrontPanelHeadphoneTopo = "FrontPanelHeadphoneTopo" ; non-localizable
KSNAME_FrontPanelMicTopo = "FrontPanelMicTopo" ; non-localizable
KSNAME_DigitalOutputTopo = "DigitalOutputTopo" ; non-localizable
KSNAME_DigitalOutput2Topo = "DigitalOutput2Topo" ; non-localizable
KSNAME_DigitalInputTopo = "DigitalInputTopo" ; non-localizable
KSNAME_MicArrayTopo = "MicArrayTopo" ; non-localizable
KSNAME_AuxInTopo = "AuxInputTopo" ; non-localizable
KSNAME_AnalogDigitalCaptureTopo = "AnalogDigitalCaptureTopo" ; non-localizable
KSNAME_AnalogDigitalCapture1Topo = "AnalogDigitalCapture1Topo" ; non-localizable
KSNAME_AnalogDigitalCapture2Topo = "AnalogDigitalCapture2Topo" ; non-localizable
KSNAME_HeadphoneTopo = "HeadphoneTopo" ; non-localizable
KSNAME_DigitalCaptureTopo = "DigitalCaptureTopo" ; non-localizable

KSNAME_eMicInWave = "eMicInWave"   ; non-localizable
KSNAME_eMicIn2Wave = "eMicIn2Wave" ; non-localizable
KSNAME_eMicIn3Wave = "eMicIn3Wave" ; non-localizable
KSNAME_eMicIn4Wave = "eMicIn4Wave" ; non-localizable
KSNAME_eMicIn5Wave = "eMicIn5Wave" ; non-localizable
KSNAME_eMicInTopo = "eMicInTopo"   ; non-localizable
KSNAME_eMicIn2Topo = "eMicIn2Topo" ; non-localizable
KSNAME_eMicIn3Topo = "eMicIn3Topo" ; non-localizable
KSNAME_eMicIn4Topo = "eMicIn4Topo" ; non-localizable
KSNAME_eMicIn5Topo = "eMicIn5Topo" ; non-localizable
 
KSNAME_eMicArrayWave = "eMicArrayWave" ; non-localizable
KSNAME_eMicArrayTopo = "eMicArrayTopo" ; non-localizable
 
KSCATEGORY_AUDIO = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}" ; non-localizable
KSCATEGORY_RENDER = "{65E8773E-8F56-11D0-A3B9-00A0C9223196}" ; non-localizable
KSCATEGORY_CAPTURE = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}" ; non-localizable
KSCATEGORY_TOPOLOGY = "{DDA54A40-1E4C-11D1-A050-405705C10000}" ; non-localizable
Proxy.CLSID = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}" ; non-localizable

HdAudGuidRearLineOutDac = "{EEF86A90-3742-4974-B8D2-5370E1C540F6}" ; non-localizable
HdAudGuidFrontHPOutDac = "{497B34AD-D67F-411c-8076-80D5B4250D67}" ; non-localizable
HdAudGuidDisableDigitalOutput = "{F06BB67D-5C2F-48ad-A307-B449E3B217D6}" ; non-localizable
HdAudGuidDigitalSpeaker = "{185FEF0D-9905-11D1-95A9-00C04FB925D3}" ; non-localizable
HdAudGuidMicDockingSelect = "{6F0B76BE-8F71-4656-828D-8E40F658ABE8}" ; non-localizable
HdAudGuidWaveOutMix = "{AA70601D-9D09-4a55-A8C9-1FC1E00EF274}" ; non-localizable
UIPATH="CNXT_AUDIO_HDA"
 
;;
;; PropertyKey GUIDS
;;
PKEY_SYSFX_Association          = "{D04E05A6-594B-4FB6-A80D-01AF5EED7D1D},0"
PKEY_SYSFX_PreMixClsid          = "{D04E05A6-594B-4FB6-A80D-01AF5EED7D1D},1"
PKEY_SYSFX_PostMixClsid         = "{D04E05A6-594B-4FB6-A80D-01AF5EED7D1D},2"
PKEY_SYSFX_UiClsid              = "{D04E05A6-594B-4FB6-A80D-01AF5EED7D1D},3"
PKEY_DisplayName                = "{B725F130-47EF-101A-A5F1-02608C9EEBAC},10"
PKEY_AudioEndpoint_Association  = "{1DA5D803-D492-4EDD-8C23-E0C0FFEE7F0E},2"
PKEY_Device_Type = "{34F9EAF0-F3FF-11DD-AC1D-B27C55D89593},0"
PKEY_Endpoint_Name = "{a45c254e-df1c-4efd-8020-67d146a850e0},2"
 
PKEY_Endpoint_ID = "{A4A2C5A8-D979-4939-B4D5-AA85D6F08162},0"
PKEY_Endpoint_Enable_LFX = "{a988f78b-07b6-4f47-9c9f-25409534cdee},0"
PKEY_Endpoint_Enable_LFX_BEAMFORMING = "{818d3b4c-2bbf-40e9-a438-9361b0ffc427},0"
PKEY_Endpoint_Enable_LFX_AEC = "{7996efb2-29c1-4898-be83-4a3646e06fac},0"
PKEY_Endpoint_Enable_GFX = "{7f73d4e1-91e3-4490-9fba-5e86680a5748},0"
PKEY_AudioEndpoint_Disable_SysFx = "{1da5d803-d492-4edd-8c23-e0c0ffee7f0e},5"
 
PKEY_AudioEndpoint_ControlPanelPageProvider = "{1DA5D803-D492-4EDD-8C23-E0C0FFEE7F0E}"
PKEY_AudioEndpoint_Supports_EventDriven_Mode = "{1DA5D803-D492-4EDD-8C23-E0C0FFEE7F0E},7"
 
;;
;; PKEY_AudioEngine_OEMFormat:  Specifies the default format that is used for rendering/capturing.
;; vartype = VT_BLOB
;;
PKEY_AudioEngine_OEMFormat = "{E4870E26-3CC5-4CD2-BA46-CA0A9A70ED04},3"
 
SYSFX_UI_CLSID      = "{17166ED2-2A70-48b8-A1AE-D5A1EC419206}"
SYSFX_PREMIX_CLSID  = "{19A120F2-EB17-4913-B7F0-C79704801726}"
SYSFX_POSTMIX_CLSID = "{C21FE761-A4DE-4060-B707-0E0C04801726}"
SYSFX_FriendlyName  = "CnxtDSP System Effect"
 
;Information for FX
; PropertyKeys
PKEY_FX_Association  = "{D04E05A6-594B-4fb6-A80D-01AF5EED7D1D},0"
PKEY_FX_PreMixClsid  = "{D04E05A6-594B-4fb6-A80D-01AF5EED7D1D},1"
PKEY_FX_PostMixClsid = "{D04E05A6-594B-4fb6-A80D-01AF5EED7D1D},2"
PKEY_FX_UiClsid      = "{D04E05A6-594B-4fb6-A80D-01AF5EED7D1D},3"
PKEY_ItemNameDisplay = "{B725F130-47EF-101A-A5F1-02608C9EEBAC},10"
 
FX_UI_CLSID      = "{5860E1C5-F95C-4a7a-8EC8-8AEF24F379A1}"
FX_PREMIX_CLSID  = "{62dc1a93-ae24-464c-a43e-452f824c4250}"
FX_POSTMIX_CLSID = "{637c490d-eee3-4c0a-973f-371958802da2}"
FX_FriendlyName  = "Microsoft Audio Home Theater Effects"
 
KSNODETYPE_ANY      = "{00000000-0000-0000-0000-000000000000}"
KSNODETYPE_SPEAKER  = "{DFF21CE1-F70F-11D0-B917-00A0C9223196}"
KSNODETYPE_HEADPHONES  		= "{DFF21CE2-F70F-11D0-B917-00A0C9223196}"
KSNODETYPE_MICROPHONE 		= "{DFF21BE1-F70F-11D0-B917-00A0C9223196}"
KSNODETYPE_LINE_CONNECTOR 		= "{DFF21FE3-F70F-11D0-B917-00A0C9223196}"
KSNODETYPE_CD_PLAYER		= "{DFF220E3-F70F-11D0-B917-00A0C9223196}"
KSNODETYPE_MICROPHONE_ARRAY 	= "{DFF21BE5-F70F-11D0-B917-00A0C9223196}"
KSNODETYPE_SPDIF_INTERFACE		= "{DFF21FE5-F70F-11D0-B917-00A0C9223196}"
;KSCATEGORY_AUDIO 			= "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"	;==>Waveout_Mix
 
REG_BINARY          = 0x00000001
REG_DWORD 		= 0x10001
 
OverrideVerbsPath =    "System\CurrentControlSet\Control\Conexant\OverrideVerbs"
